BUILDING AUTOMATION SYSTEM (BAS) MONITORING PROCESS

Created by ChecklistGuro (https://checklistguro.com)

[ ] Fetch Sensor Telemetry: Retrieve latest temperature, humidity, and pressure readings from the BAS sensor data model.
[ ] Calculate Average Daily Temperature: Aggregate the retrieved sensor readings to find the mean temperature over the last 24 hours.
[ ] Check Threshold Deviation: Compare the average temperature against the predefined setpoint to calculate the degree of deviation.
[ ] Create Alert Incident: Create a new entry in the 'Incidents' data model when a deviation exceeds the allowed tolerance.
[ ] Update Equipment Status: Update the status of the specific HVAC unit in the 'Equipment' data model to 'Warning' or 'Critical'.
[ ] Assign Technician Investigation: Create a task for the On-call Maintenance Engineer to inspect the hardware.
[ ] Visual Inspection Checklist: A set of sub-tasks for the technician: check physical wiring, verify power supply, and inspect sensor calibration.
[ ] Notify Facility Manager: Send an automated email to the Facility Manager summarizing the critical deviation and the created incident.
[ ] Urgent Alert SMS: Send a high-priority SMS to the Lead Engineer for immediate-action-required-threshold-breach.
[ ] Retrieve Maintenance Logs: Get the history of previous repairs for the affected equipment to identify recurring patterns.
[ ] Log Incident Resolution: Update the 'Incident' entry with the technician's findings and resolution notes once the task is complete.
[ ] Generate Weekly Performance Report: Create a summary report aggregating all incidents, deviations, and resolution times for the weekly management review.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/facility-management/building-automation-system-bas-monitoring-process
(Click "Install Template" to launch your digital inspection tool immediately)