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Created by ChecklistGuro (https://checklistguro.com)


--- ROOFING & PARAPET INSPECTION ---
[ ] Inspection Date
[ ] Roof Section/Zone ID
[ ] Roof Membrane Condition (Excellent, Good, Fair - Monitoring Required, Poor - Urgent Repair Needed)
[ ] Observed Defects (Cracking/Tearing, Ponding Water, Blistering, Debris Accumulation, Damaged Flashing)
[ ] Estimated Depth of Ponding (inches)
[ ] Photo Evidence of Defect
[ ] Detailed Observations & Repair Recommendations
[ ] Inspector Signature

--- EXTERIOR WALL & CLADDING ASSESSMENT ---
[ ] Cladding Material Type (Brick/Masonry, EIFS (Exterior Insulation and Finish System), Metal Panels, Stucco, Concrete/Precast, Fiber Cement Siding, Other)
[ ] Observed Deficiencies (Cracks or Fissures, Spalling or Chipping, Discoloration/Staining, Loose or Missing Panels, Efflorescence, Impact Damage)
[ ] Detailed Observation Notes
[ ] Defect Photo Documentation
[ ] Estimated Severity Score (1-10)
[ ] Inspector Verification

--- WINDOW, GLAZING & FENESTRATION REVIEW ---
[ ] Window Frame Condition (Excellent, Good, Fair (Minor Wear), Poor (Needs Repair), Critical (Immediate Action Required))
[ ] Observed Defects (Cracked Glass, Broken Seal/Fogging, Failed Gaskets/Weatherstripping, Corroded Frames, Loose Hardware, Water Leaks Detected)
[ ] Detailed Defect Description
[ ] Photo Evidence of Glazing/Frame Condition
[ ] Estimated Repair Cost (USD)

--- SEALANTS, CAULKING & JOINT INSPECTION ---
[ ] Sealant Condition Status (Intact & Functional, Cracked or Degraded, Missing or Detached, Evidence of Water Ingress)
[ ] Observations of Joint Deterioration
[ ] Identified Issues (Cracking, Adhesion Failure, Shrinkage, Surface Erosion, Biological Growth (Mold/Algae))
[ ] Photo Evidence of Sealant Failure
[ ] Estimated Linear Feet Requiring Replacement
[ ] Date of Inspection

--- STRUCTURAL INTEGRITY & LOAD-BEARING ELEMENTS ---
[ ] Structural Element Component Type (Lintel, Support Column, Reinforced Concrete, Steel Beam, Load-bearing Masonry)
[ ] Structural Condition Status (Intact - No visible defects, Minor Cracking/Wear, Moderate Damage - Requires Repair, Critical Failure - Immediate Action Required)
[ ] Detailed Observation of Cracks or Degradation
[ ] Evidence Photo of Structural Defect
[ ] Inspector Verification

--- MOISTURE & WATER INGRESS INDICATORS ---
[ ] Presence of Efflorescence on Masonry (None Detected, Minor (Light White Residue), , Severe (Structural Concern))
[ ] Observed Moisture Indicators (Visible Water Staining, Visible Mold or Mildew Growth, Surface Dampness/Wetness, Peeling or Bubbling Paint, Spalling Concrete)
[ ] Description of Damage Location and Severity
[ ] Photographic Evidence of Ingress
[ ] Specific Wall/Facade Area Affected

--- DRAINAGE & WATER MANAGEMENT SYSTEMS ---
[ ] Gutter & Downspout Condition (Clear and Functional, Debris Accumulation Detected, Damaged or Corroded, Disconnected or Leaking)
[ ] Drainage Blockage Locations
[ ] Observed Water Accumulation (in mm/inches)
[ ] Photo Documentation of Drainage Issues
[ ] Detailed Observations & Maintenance Recommendations
[ ] Inspector Verification

--- METALWORK & HARDWARE INSPECTION ---
[ ] Component Condition Status (Good - No action required, Fair - Requires monitoring, Poor - Immediate repair needed, Critical - Structural risk)
[ ] Identified Issues (Surface Rust/Oxidation, Loose or Missing Fasteners, Corroded Hardware, Deformed or Warped Metal, Degraded Protective Coating)
[ ] Detailed Observations
[ ] Evidence Photos
[ ] Inspector Verification

--- THERMAL BRIDGING & INSULATION AUDIT ---
[ ] Inspection Date
[ ] Building Zone/Area Inspected
[ ] Visible Thermal Anomalies Detected (None Detected, Minor Heat Loss, Significant Thermal Bridge, Insulation Degradation Observed)
[ ] Description of Observed Thermal Gaps or Insulation Voids
[ ] Thermal Imaging/Infrared Thermography Photos
[ ] Estimated Temperature Differential (Delta T)
[ ] Inspector Verification

--- SUMMARY & REMEDIATION PRIORITY ---
[ ] Inspection Completion Date
[ ] Overall Building Condition Rating (Critical - Immediate Action Required, Fair - Maintenance Required, Good - Stable, Excellent - No Action Needed)
[ ] Detailed Remediation Summary
[ ] Identified High-Priority Issues (Structural Cracking, Water Leakage/Moisture, Sealant/Caulking Failure, Corrosion/Oxidation, Material Degradation)
[ ] Photographic Evidence of Critical Defects
[ ] Inspector Signature
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