COLUMN/BEAM ALIGNMENT AND PLUMBNESS CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- COLUMN BASE AND FOOTING ALIGNMENT ---
[ ] Column Base to Footing Offset (East-West)
[ ] Column Base to Footing Offset (North-South)
[ ] Column Base to Footing Offset (Vertical)
[ ] Footing Alignment Verification Method (Tape Measure, Laser Level, Transit/Theodolite, Other (Specify in Long Text))
[ ] Detailed Description of Alignment Verification Process (if 'Other' selected above)
[ ] Tolerance for Base to Footing Offset (East-West)
[ ] Tolerance for Base to Footing Offset (North-South)
[ ] Tolerance for Base to Footing Offset (Vertical)
[ ] Status of Alignment (Aligned, Minor Adjustment Required, Major Adjustment Required)

--- COLUMN VERTICALITY (PLUMBNESS) ---
[ ] Column ID
[ ] Verticality Deviation (at base)
[ ] Verticality Deviation (at midpoint)
[ ] Verticality Deviation (at top)
[ ] Measurement Method (Plumb Bob, Laser Level, Spirit Level, Total Station)
[ ] Within Tolerance? (Yes, No)
[ ] Notes / Observations
[ ] Plumbness Photo
[ ] Tolerance Limit (inches/mm)

--- COLUMN HEAD ALIGNMENT ---
[ ] Column Head Elevation (Relative to Datum)
[ ] Discrepancy from Design Elevation
[ ] Column Head Alignment Method (Laser Level, Spirit Level & Tape, Plumb Bob)
[ ] Horizontal Offset from Design Line (Column A)
[ ] Horizontal Offset from Design Line (Column B)
[ ] Column Head Alignment Status (Within Tolerance, Outside Tolerance - Corrective Action Required)
[ ] Notes on Column Head Alignment (If Applicable)
[ ] Photo Evidence of Column Head Alignment

--- BEAM ALIGNMENT TO COLUMN ---
[ ] Column Line Offset (mm/inches)
[ ] Beam Centerline Offset from Column Face (mm/inches)
[ ] Beam Top Elevation Relative to Column Top (mm/inches)
[ ] Beam Seating Condition (Proper Seat, Minor Adjustment Required, Significant Adjustment Required)
[ ] Beam Levelness Verification Method (Spirit Level, Laser Level, Digital Level)
[ ] Notes on Alignment & Seating (if adjustments needed)
[ ] Inspector Signature

--- BEAM LEVELNESS ---
[ ] Levelness Check Point 1 - Elevation (ft/in)
[ ] Levelness Check Point 1 - Deviation from Design (in)
[ ] Levelness Check Point 2 - Elevation (ft/in)
[ ] Levelness Check Point 2 - Deviation from Design (in)
[ ] Maximum Allowable Deviation (in)
[ ] Levelness Within Tolerance? (Yes, No)
[ ] Notes/Corrective Actions (if applicable)
[ ] Supporting Photos/Level Readings

--- COLUMN/BEAM CONNECTION ALIGNMENT ---
[ ] Column-Beam Intersection Offset (Horizontal)
[ ] Column-Beam Intersection Offset (Vertical)
[ ] Bolt Hole Misalignment (Max. Allowed)
[ ] Welding Gap (If Applicable)
[ ] Connection Type (Bolted, Welded, Pinned)
[ ] Bolt Pattern Verification (Correct, Incorrect - Requires Adjustment)
[ ] Notes on Connection Alignment
[ ] Inspector Signature

--- REVIEW OF SURVEY DATA & REFERENCE POINTS ---
[ ] Survey Data Reviewed? (Yes, No)
[ ] Survey Point Elevation (Reference)
[ ] Grid North Deviation (if applicable)
[ ] Description of Survey Data Used
[ ] Location of Survey Control Points
[ ] Date of Survey Data

--- CORRECTIONS AND RE-CHECKS ---
[ ] Description of Correction(s) Required
[ ] Amount of Adjustment (mm/inches)
[ ] Date of Correction
[ ] Time of Correction
[ ] Method Used for Correction
[ ] Re-check Measurement (mm/inches)
[ ] Correction Status (Complete, Partial, Not Yet Addressed)
[ ] Corrector's Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/column-beam-alignment-and-plumbness-checklist
(Click "Install Template" to launch your digital inspection tool immediately)