CONSTRUCTION SCAFFOLDING SETUP & STABILITY CHECKLIST 2026
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--- PRE-INSTALLATION & SITE ASSESSMENT ---
[ ] Inspection Date
[ ] Work Site/Project Location
[ ] Ground Surface Condition (Concrete/Pavement, Compacted Soil, Asphalt, Unstable/Loose Dirt)
[ ] Pre-Existing Site Hazards Identified (Overhead Power Lines, Nearby Pedestrian Traffic, Adjacent Structures/Scaffolding, Underground Utilities, High Wind/Weather Risks)
[ ] Hazard Mitigation Actions Taken
[ ] Site Supervisor Verification

--- BASE SUPPORT & FOUNDATION STABILITY ---
[ ] Ground Surface Type (Concrete/Asphalt, Soil/Dirt, Gravel/Crushed Stone, Pavement/Slab)
[ ] Mudsill Condition (Secure and Level, Unstable/Sinking, Insufficient Size)
[ ] Base Plate & Jack Installation Status (Fully Installed & Level, Missing Components, Improperly Threaded)
[ ] Foundation Deficiencies Noted
[ ] Photo of Base/Sill Setup
[ ] Inspector Verification

--- STRUCTURAL FRAMEWORK & COMPONENT INTEGRITY ---
[ ] Standard & Ledger Condition (Excellent (No visible damage), Fair (Minor surface rust/wear), Defective (Requires immediate replacement))
[ ] Checked Components (Vertical Standards, Horizontal Ledgers, Transoms, Cross Bracing, Swivel/Fixed Couplers)
[ ] Defect Details & Observations
[ ] Component Integrity Photos
[ ] Inspector Verification

--- PLANKING & WORKING PLATFORM SAFETY ---
[ ] Plank Material Condition (Intact/No Visible Damage, Damaged/Cracked - Requires Replacement, Decayed/Rotting (Wood only))
[ ] Plank Overlap Verification (Minimum 6-12 inch overlap achieved, Insufficient overlap)
[ ] Gap Width Between Planks (inches)
[ ] Platform Hazards Identified (Gaps larger than 1 inch, Loose or unsecured planks, Slip hazards (oil, mud, ice), Protruding nails or splinters)
[ ] Photo Evidence of Platform Surface
[ ] Corrective Actions Taken

--- GUARDRAIL & FALL PROTECTION SYSTEMS ---
[ ] Top Rail Height Verification (Meets regulatory height requirements (42 inches +/- 3 inches), Does not meet height requirements)
[ ] Mid-Rail Installation Status (Installed and secure, Missing or loose)
[ ] Toe Board Integrity (Present and securely fastened, Missing or gaps detected)
[ ] Identified Fall Hazards (Unprotected edges, Missing mid-rails, Inadequate toe boards, Unsecured guardrail connections)
[ ] Deficiency Notes & Corrective Actions
[ ] Photo Evidence of Guardrail Setup
[ ] Safety Inspector Verification

--- ACCESS & EGRESS VERIFICATION ---
[ ] Primary Access Method (Internal Ladder, External Ladder, Stair Tower, Scaffold Stairway)
[ ] Ladder/Stairway Condition (Secure and Stable, Needs Repair, Unsafe/Do Not Use)
[ ] Safety Features Verified (Clear of Obstructions, Handrails Installed, Three-Point Contact Maintained, Non-Slip Surfaces Present)
[ ] Access Issues or Deficiencies Noted
[ ] Inspector Verification

--- LOAD CAPACITY & WEIGHT DISTRIBUTION ---
[ ] Maximum Rated Load Capacity (kg/lbs)
[ ] Scaffold Load Classification (Light Duty, Medium Duty, Heavy Duty)
[ ] Weight Distribution Checks Completed (Load-bearing surface verified, No heavy materials stacked on single plank, Equipment weight accounted for, Center of gravity verified)
[ ] Load Distribution Observations
[ ] Load Calculation Documentation

--- TIES, BRACING, AND STABILITY ANCHORING ---
[ ] Wall Tie Integrity Status (Securely Anchored, Requires Immediate Attention, Not Installed)
[ ] Types of Bracing Verified (Cross Bracing, Diagonal Bracing, Horizontal Bracing, Structural Ties)
[ ] Number of Verified Anchor Points
[ ] Notes on Anchoring Defects or Observations
[ ] Photo Evidence of Tie & Brace Connections
[ ] Safety Inspector Verification

--- ENVIRONMENTAL & SAFETY SIGNAGE ---
[ ] Scaffold Tag Status (Green (Safe for Use), Yellow (Caution - Modified), Red (Danger - Do Not Use))
[ ] Required Signage Present (Maximum Load Capacity Sign, PPE Requirements Sign, Fall Hazard Warning, Authorized Personnel Only)
[ ] Missing Signage Notes
[ ] Last Signage Inspection Date
[ ] Photo of Completed Signage Installation
[ ] Safety Officer Verification

--- END OF TEMPLATE ---
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