CROP YIELD MONITORING AND ANALYSIS WORKFLOW

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Field Sensor Data: Fetch the latest soil moisture, temperature, and humidity readings from the Sensor Data Model.
[ ] Fetch Historical Yield Records: Retrieve previous season's yield data for the specific field plots being analyzed.
[ ] Calculate Average Soil Moisture: Calculate the average moisture level from all retrieved sensor entries to determine drought risk.
[ ] Compute Yield Gap Index: Calculate the difference between the current predicted yield and the historical average yield.
[ ] Create Analysis Report Entry: Create a new record in the Yield Analysis Model containing the calculated metrics and findings.
[ ] Assign Agronomist Review: Create a task for the assigned Agronomist to manually verify the automated findings.
[ ] Retrieve Agronomist Feedback: Fetch the notes and verification status entered by the Agronomist in their task completion.
[ ] Determine Risk Level: Use a formula to categorize risk (Low, Medium, High) based on moisture and yield gap values.
[ ] Update Field Health Status: Update the 'Status' property in the Field Data Model based on the calculated Risk Level.
[ ] Generate Remediation Task: If risk is High, create a task for the Farm Manager to implement irrigation or fertilization.
[ ] Generate Seasonal Yield Report: Compile all processed analysis entries into a comprehensive seasonal performance report.
[ ] Notify Stakeholders: Send an email summary of the yield analysis and risk alerts to the Farm Owners.
[ ] Urgent Alert SMS: Send an SMS notification to the Field Supervisor if moisture levels drop below a critical threshold.
[ ] Cleanup Temporary Calculations: Delete temporary calculation logs once the final Analysis Report has been successfully created.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/farm-management/crop-yield-monitoring-and-analysis-workflow
(Click "Install Template" to launch your digital inspection tool immediately)