DRYWALL INSTALLATION AND FASTENING CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-INSTALLATION & FRAMING ---
[ ] Framing Stud Spacing (inches)
[ ] Framing Thickness (inches)
[ ] Framing Type (Wood, Metal)
[ ] Wall Straightness - Assessment (Within Tolerance, Minor Correction Needed, Significant Correction Needed)
[ ] Notes on Framing Condition/Corrections
[ ] Framing Inspection Date
[ ] Floor Level Difference (inches) - Check for Level

--- DRYWALL MATERIAL INSPECTION ---
[ ] Drywall Type Verification (Regular (1/2"), 5/8", Fire-Rated, Moisture-Resistant (Greenboard), Mold-Resistant)
[ ] Sheet Thickness (inches)
[ ] Defect Identification (Bends/Curls, Cracks, Chips/Damage, Stains/Discoloration, None, Other (Specify in Long Text))
[ ] Defect Description (if applicable)
[ ] Quantity of Sheets Received
[ ] Quantity of Sheets Used
[ ] Condition of Packaging (Intact, Damaged, Compromised)

--- DRYWALL LAYOUT & CUTTING ---
[ ] Project Drawing Review Notes:
[ ] Drywall Sheet Size (Nominal): (4' x 8', 4' x 10', Other (Specify))
[ ] Number of Drywall Sheets to Cut:
[ ] Cutting Plan Notes (layout, waste reduction, efficiency):
[ ] Cutting Strategy: (Staggered, Alternating, Other (Specify))
[ ] Estimated Drywall Waste (sq ft):
[ ] Cutting Plan Diagram (if applicable):

--- DRYWALL HANGING - GENERAL ---
[ ] Drywall Orientation (Vertical or Horizontal) (Vertical, Horizontal)
[ ] Number of Drywall Sheets Installed
[ ] Staggered Joint Placement (Yes/No) (Yes, No)
[ ] Maximum Sheet Length (feet)
[ ] Notes on Joint Alignment and Overlap
[ ] Drywall Edge Treatment (Tapered, Square) (Tapered, Square)
[ ] Description of any issues or adjustments made during hanging

--- FASTENER SPACING & TYPE ---
[ ] Framing Type? (Wood, Metal)
[ ] Drywall Thickness (inches)
[ ] Fastener Type? (Drywall Screws, Annular Thread Screws, Other (Specify))
[ ] If 'Other' fastener type selected, specify:
[ ] Maximum Screw Spacing (inches) - Wood Framing
[ ] Maximum Screw Spacing (inches) - Metal Framing
[ ] Edge Distance (inches) - Minimum Distance from Drywall Edge
[ ] Screw Depth (inches)
[ ] Screw head orientation (Slightly recessed, Flush, Slightly protruding)

--- JOINT TREATMENT - TAPING & MUDDING ---
[ ] Number of Taping Coats Applied
[ ] Number of Mudding Coats Applied
[ ] Mud Type Used (e.g., All-Purpose, Lightweight) (All-Purpose, Lightweight, Setting-Type)
[ ] Taping Technique Used (Machine Taping, Hand Taping)
[ ] Notes on Joint Condition Before Taping/Mudding
[ ] Joint Compound Drying Time Adhered To? (Yes, No, N/A)
[ ] Specific Issues/Corrections Made During Taping/Mudding (e.g., cracking, pinholes)
[ ] Sanding Required? (Yes, No)

--- CORNER TREATMENT ---
[ ] Corner Type (Inside Corner, Outside Corner, Bullnose Corner)
[ ] Corner Compound Coats (Inside Corners)
[ ] Corner Compound Coats (Outside Corners)
[ ] Bead Type (Outside Corners) (Metal L-Bead, Paper/Mesh Bead, None (Hand-beaded))
[ ] Notes on Corner Treatment
[ ] Sanding Method (Corners) (Hand Sanding, Power Sanding, Combination)
[ ] Dry Time (Between Coats)

--- FINAL INSPECTION & CLEANUP ---
[ ] Overall Drywall Finish Appearance (Excellent - No visible imperfections, Good - Minor imperfections easily corrected, Fair - Noticeable imperfections requiring attention, Poor - Significant imperfections, rework needed)
[ ] Number of Joint Compound Coats Applied
[ ] Joint Compound Drying Time Observed (Complies with Manufacturer's Recommendations, Slightly longer than recommended, Significantly longer than recommended)
[ ] Notes on Observed Defects/Concerns
[ ] Fastener Head Embedment (Optimal - Slightly depressed, Acceptable - Flush, Requires Adjustment - Protruding)
[ ] Photographic Evidence (if applicable)
[ ] Area Cleanliness (Clean and free of debris, Minor cleanup required, Requires significant cleanup)
[ ] Date of Final Inspection

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/drywall-installation-and-fastening-checklist
(Click "Install Template" to launch your digital inspection tool immediately)