ELECTRICAL PANEL AND CIRCUITRY INSPECTION CHECKLIST TEMPLATE 2026
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--- GENERAL PANEL INTEGRITY AND HOUSING ---
[ ] Inspection Date
[ ] Panel Room/Building Location
[ ] Enclosure Condition (Excellent, Good, Fair, Poor)
[ ] Visible Damage Detected (Corrosion/Rust, Dents or Deformations, Missing Screws/Fasteners, Incomplete Cover/Dead Front, None)
[ ] Damage Observations and Notes
[ ] Photo of Panel Enclosure
[ ] Inspector Signature

--- CIRCUIT BREAKERS AND OVERCURRENT PROTECTION ---
[ ] Breaker Condition Status (Functional/Normal, Faulty/Damaged, Requires Immediate Replacement)
[ ] Observed Temperature (Celsius)
[ ] Visible Signs of Stress (Discoloration/Charring, Arc Marks, Corrosion, Debris/Dust Accumulation)
[ ] Detailed Defect Description
[ ] Breaker Thermal Image or Photo
[ ] Inspector Verification

--- WIRING AND CONDUCTOR CONDITION ---
[ ] Insulation Condition (Intact, Frayed/Damaged, Brittle/Cracked, Signs of Heat/Burning)
[ ] Observed Temperature (Celsius)
[ ] Observed Defects (Exposed Copper, Corrosion, Improper Wire Gauge, Overcrowded Wires)
[ ] Detailed Observations and Notes
[ ] Wiring Damage Photo Evidence

--- TERMINATIONS AND CONNECTIONS ---
[ ] Connection Tightness Status (Secure, Loose/Requires Tightening, Corroded/Damaged)
[ ] Observed Oxidation or Corrosion
[ ] Detected Temperature Reading (Celsius)
[ ] Identified Issues (Loose Terminal Screws, Exposed Copper, Discolored Insulation, Improper Wire Stripping)
[ ] Detailed Observations and Remediation Notes
[ ] Photo Evidence of Connections

--- GROUNDING AND BONDING VERIFICATION ---
[ ] Grounding Electrode Conductor Condition (Excellent (No corrosion or damage), Fair (Minor oxidation noted), Poor (Heavy corrosion or damage), N/A)
[ ] Main Bonding Jumper Presence (Present and Secure, Missing or Loose, Not Applicable)
[ ] Measured Ground Resistance (Ohms)
[ ] Identified Bonding Issues (Loose terminal screw, Corroded connection, Incomplete bonding to metallic piping, Disconnected ground wire)
[ ] Photo Evidence of Grounding Connections
[ ] Detailed Observations and Rectification Notes

--- LABELING AND CIRCUIT IDENTIFICATION ---
[ ] Circuit Directory Status (Complete and Accurate, Incomplete/Missing Labels, Illegible/Unreadable, Outdated/Non-compliant)
[ ] Missing Circuit Description
[ ] Last Directory Update Date
[ ] Photo of Circuit Directory
[ ] Inspector Verification

--- ENVIRONMENTAL AND CLEARANCE COMPLIANCE ---
[ ] Working Clearance Maintained (Yes, No, N/A)
[ ] Obstruction Check (Clear of storage/combustibles, Obstructed by debris/items)
[ ] Distance to Nearest Obstruction (ft)
[ ] Clearance Deficiencies Noted
[ ] Photo Documentation of Panel Area
[ ] Inspector Verification

--- END OF TEMPLATE ---
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