FRAMING LAYOUT VERIFICATION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL SITE CONDITIONS & DOCUMENTATION ---
[ ] Date of Layout Verification
[ ] Time of Layout Verification
[ ] Project Location
[ ] Weather Conditions During Layout
[ ] Drawing Set Used for Verification (Revision A, Revision B, Revision C, Other (Specify))
[ ] Copy of Approved Framing Layout Plans
[ ] Permit Status (Approved, Pending, Not Required)
[ ] Layout Verification Company

--- FOUNDATION VERIFICATION ---
[ ] Foundation Elevation (Existing)
[ ] Foundation Elevation (Proposed)
[ ] Foundation Levelness Deviation (Max)
[ ] Foundation Type (Poured Concrete, Concrete Block, Crawlspace, Slab-on-Grade)
[ ] Rebar Size Verification (Verified, Not Verified)
[ ] Rebar Spacing (Inches)
[ ] Comments/Observations (Foundation)
[ ] Foundation As-Built Drawing (Uploaded)

--- WALL LAYOUT VERIFICATION ---
[ ] Wall Offset from Property Line (East)
[ ] Wall Offset from Property Line (West)
[ ] Wall Length (Wall 1)
[ ] Wall Length (Wall 2)
[ ] Wall Thickness (Check consistency)
[ ] Wall Alignment (Consistent with plans?) (Yes, No, NA)
[ ] Interior Wall Location (Consistent with plans?) (Yes, No, NA)
[ ] Notes on Wall Layout Discrepancies (if any)

--- BEAM AND HEADER LAYOUT ---
[ ] Beam Elevation (Top of Beam)
[ ] Header Height (Bottom of Joist)
[ ] Beam Width
[ ] Header Width
[ ] Beam/Header Material Type (SPF Lumber, LVL, Glulam, Steel, Other)
[ ] Bearing Length (Beam)
[ ] Bearing Length (Header)
[ ] Connection Type (Nail, Bolt, Screw, Other)
[ ] Notes/Comments

--- DOOR AND WINDOW OPENINGS ---
[ ] Window Sill Height (above finished floor)
[ ] Window Header Height (above finished floor)
[ ] Door Head Height (above finished floor)
[ ] Door Sill Height (above finished floor)
[ ] Window Width (actual measurement)
[ ] Window Height (actual measurement)
[ ] Door Width (actual measurement)
[ ] Door Height (actual measurement)
[ ] Window Opening Squareness (Square, Slightly Out of Square, Significantly Out of Square)
[ ] Notes/Corrections Required (if any)

--- STAIRWAY LAYOUT (IF APPLICABLE) ---
[ ] Total Rise (inches)
[ ] Total Run (inches)
[ ] Rise per Step (inches)
[ ] Run per Step (inches)
[ ] Nosing (inches)
[ ] Stairway Type (Straight Run, Winding, Spiral, Split (Double) Stringer)
[ ] Headroom (minimum 9ft or as per code) (inches)
[ ] Handrail Presence (Yes, No)
[ ] Handrail Location/Details (if applicable)

--- SHEAR WALL/BEARING WALL LAYOUT (IF APPLICABLE) ---
[ ] Shear Wall/Bearing Wall Layout Drawing Version (Latest Revision, Previous Revision)
[ ] Shear Wall Thickness (inches)
[ ] Bearing Wall Thickness (inches)
[ ] Shear Wall Type (per structural drawings) (Plywood Sheathed, OSB Sheathed, Composite Sheathing, Other (Specify in Long Text))
[ ] If 'Other' Shear Wall Type Selected, Please Specify:
[ ] Nail Spacing (inches) - Horizontal
[ ] Nail Spacing (inches) - Vertical
[ ] Reinforcement Check (Select all that apply) (Vertical Rebar Present, Horizontal Rebar Present, Shear Wall Anchors Installed, None Required)
[ ] Location of Shear Wall Detail for verification

--- FINAL REVIEW & SIGN-OFF ---
[ ] Date of Final Verification
[ ] Time of Final Verification
[ ] Summary of Findings/Discrepancies
[ ] Corrective Actions Taken
[ ] Overall Verification Status (Approved, Conditional Approval (See Notes), Rejected (See Notes))
[ ] Inspector Name
[ ] Inspector Signature
[ ] Revisions/Rework Required (if any)
[ ] Supporting Photos/Documents (if applicable)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/framing-layout-verification-checklist
(Click "Install Template" to launch your digital inspection tool immediately)