GEOTHERMAL ENERGY EXTRACTION PROCESS

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Site Geological Data: Fetch existing geological survey data and temperature readings from the Site Analysis data model.
[ ] Calculate Thermal Potential: Calculate the estimated energy output using retrieved temperature and pressure data.
[ ] Create Feasibility Report Entry: Create a new record in the Feasibility Studies data model with the calculated thermal potential.
[ ] Assign Drilling Permit Review: Create a task for the Legal Department to review environmental and drilling permits.
[ ] Check Permit Status: Retrieve the status of regulatory permits from the Regulatory Compliance data model.
[ ] Update Site Readiness Status: Update the Site Readiness data model to 'Ready for Drilling' once permits are confirmed.
[ ] Execute Borehole Drilling: Create a task for the Engineering Team to initiate the drilling operations.
[ ] Log Drilling Parameters: Create new entries in the Drilling Log data model for depth, pressure, and temperature encountered.
[ ] Aggregate Drilling Pressure Data: Calculate the maximum pressure encountered during the drilling phase from the Drilling Log entries.
[ ] Assess Pressure Risk: Compare the maximum pressure against safety thresholds to determine if reinforcement is needed.
[ ] Well Casing Installation: Create a task for the Field Technicians to install well casing based on the pressure assessment.
[ ] Update Well Integrity Record: Update the Well Infrastructure data model with the installation timestamp and casing specifications.
[ ] Retrieve Flow Rate Data: Fetch fluid flow rate data from the Production Monitoring data model.
[ ] Calculate Average Flow Rate: Calculate the average flow rate over the last 24 hours to ensure steady-state production.
[ ] Notify Production Manager: Send an email notification to the Production Manager regarding the daily flow rate stability.
[ ] Equipment Maintenance Check: Create a periodic maintenance task for the heat exchanger and turbine components.
[ ] Update Maintenance Log: Update the Maintenance Schedule data model to reflect the completion of the check.
[ ] Generate Monthly Production Report: Create a comprehensive performance report summarizing energy output, flow rates, and downtime.
[ ] Alert Emergency Response: Send an SMS alert to the Emergency Response Team if pressure thresholds exceed safety limits.
[ ] Clear Temporary Sensor Logs: Delete temporary, high-frequency sensor data entries once they have been aggregated into long-term storage.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/energy/geothermal-energy-extraction-process
(Click "Install Template" to launch your digital inspection tool immediately)