HYDRAULIC SYSTEM LEAKAGE CHECK

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-INSPECTION & SAFETY ---
[ ] Inspection Date
[ ] Inspection Start Time
[ ] Weather Conditions (Clear, Cloudy, Rain, Snow, Foggy)
[ ] PPE Used (Select All That Apply) (Safety Glasses, Gloves, Hearing Protection, Steel-Toe Boots)
[ ] Brief Description of Equipment Being Inspected
[ ] Equipment Status Before Inspection (Operational, Not Operational)

--- VISUAL INSPECTION - RESERVOIR & FILL POINTS ---
[ ] Reservoir Condition Notes
[ ] Reservoir Leakage? (None, Minor Drip, Moderate Leak, Severe Leak)
[ ] Fill Point Condition (Good, Cracked, Leaking, Damaged)
[ ] Reservoir Fluid Level (inches)
[ ] Filler Cap Condition Notes
[ ] Fluid Type Correct? (Yes, No, Unknown)

--- VISUAL INSPECTION - HYDRAULIC LINES & FITTINGS ---
[ ] Condition of Hydraulic Lines (General) (Excellent - No visible wear, Good - Minor wear, no leaks, Fair - Moderate wear, possible minor leaks, Poor - Significant wear, evident leaks)
[ ] Condition of Fittings (Overall) (Secure and Tight, Slightly Loose, Loose - Requires Adjustment, Leaking - Requires Replacement)
[ ] Affected Line Types (if leaks present) (High-Pressure Lines, Low-Pressure Lines, Return Lines, Suction Lines, None - No Leaks Observed)
[ ] Specific Location of Leaks (if present)
[ ] Leak Severity (if present) (Drip, Stream, Spray)
[ ] Estimated Leak Rate (drops/minute, if possible)
[ ] Photo of Affected Lines/Fittings (if leaks present)

--- VISUAL INSPECTION - CYLINDERS & MOTORS ---
[ ] Describe any visible signs of leakage from Cylinder 1 (e.g., drips, puddles, residue).
[ ] Cylinder 1 Leak Severity (if present) (None, Minor, Moderate, Severe)
[ ] Describe any visible signs of leakage from Cylinder 2 (e.g., drips, puddles, residue).
[ ] Cylinder 2 Leak Severity (if present) (None, Minor, Moderate, Severe)
[ ] Describe any visible signs of leakage from Motor 1 (e.g., drips, puddles, residue).
[ ] Motor 1 Leak Severity (if present) (None, Minor, Moderate, Severe)
[ ] Describe any visible signs of leakage from Motor 2 (e.g., drips, puddles, residue).
[ ] Motor 2 Leak Severity (if present) (None, Minor, Moderate, Severe)

--- PRESSURE TEST (OPTIONAL) ---
[ ] Test Pressure (PSI)
[ ] Hold Time (Seconds)
[ ] Pressure Drop (PSI)
[ ] Description of Test Setup
[ ] Observations During Pressure Test
[ ] Test Result (Pass, Fail, Inconclusive)

--- POST-INSPECTION & DOCUMENTATION ---
[ ] Overall System Condition Notes
[ ] Leakage Rate (Drops/Minute) - Overall
[ ] Leak Locations (Select all that apply) (Reservoir, Hydraulic Lines, Cylinders, Motors, Fittings, Other (Specify in notes))
[ ] Detailed Description of Found Leaks
[ ] Estimated Repair Time (Hours)
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Inspection Result (No Leaks Found, Minor Leaks (No Immediate Action Required), Moderate Leaks (Repair Recommended), Severe Leaks (Immediate Repair Required))
[ ] Photos of Leaks (Optional)
[ ] Inspector Name

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/agriculture/hydraulic-system-leakage-check
(Click "Install Template" to launch your digital inspection tool immediately)