LABORATORY EQUIPMENT INSPECTION WORKFLOW: GLP/GLP COMPLIANCE AND CALIBRATION MANAGEMENT

Created by ChecklistGuro (https://checklistguro.com)

[ ] Initiate Inspection Task: Create the initial inspection task for the specific piece of laboratory equipment.
[ ] Retrieve Equipment Serial Number: Get the unique identifier and details for the asset needing inspection (e.g., spectrophotometer, pH meter).
[ ] Get Associated Calibration Schedule: Retrieve the next due date and required calibration standard from the asset master record.
[ ] Assign Calibration Task to Technician: Automatically assign the necessary inspection task to the qualified lab technician.
[ ] Record Inspection Findings: Input inspection results, observations, and readings into the designated data model.
[ ] Calculate Calibration Due Date: Determine the next service interval based on current date and manufacturer recommendations (e.g., date + 1 year).
[ ] Generate Calibration Report Draft: Automatically generate the preliminary report structure using collected data.
[ ] Notify Manager of Task Completion: Send an automated email notification to the Lab Manager upon task completion, attaching preliminary results.
[ ] Submit Finalized Calibration Record: Submit the final, signed-off record of the calibration and inspection results for record-keeping.
[ ] Calculate Overall Equipment Health Score: Aggregate multiple inspection data points to generate a composite health score for the equipment.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/inspection-management/laboratory-equipment-inspection-workflow-glp-glp-compliance-and-calibration-management
(Click "Install Template" to launch your digital inspection tool immediately)