MINING PPE COMPLIANCE CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-SHIFT INSPECTION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Employee ID
[ ] Overall PPE Condition (Excellent, Good, Fair, Poor)
[ ] Comments/Observations
[ ] Inspector Signature

--- HEAD PROTECTION (HARD HATS) ---
[ ] Hard Hat Condition (Good, Fair, Damaged - Remove from Service)
[ ] Suspension Comfort Rating (1-5, 5=Most Comfortable)
[ ] Chin Strap Secured? (Yes, No)
[ ] Any Damage Observed (Cracks, Dents)?
[ ] Last Hard Hat Replacement Date

--- EYE AND FACE PROTECTION ---
[ ] Type of Eye Protection Worn (Safety Glasses, Goggles, Face Shield, Combination (Glasses & Shield))
[ ] Condition of Lenses (Clear, Scratched, Fogged, Cracked/Broken)
[ ] Scratch Depth (mm, if applicable)
[ ] Face Shield Condition (if applicable) (Clear, Scratched, Cracked/Broken)
[ ] Last Inspection Date

--- RESPIRATORY PROTECTION ---
[ ] Respirator Type Required? (Not Required, Dust Mask, Half-Face Respirator, Full-Face Respirator, SCBA)
[ ] Cartridge/Filter Type (if applicable) (P100, N95, Organic Vapor, Acid Gas, Combination)
[ ] Cartridge/Filter Replacement Date
[ ] Number of Cartridges/Filters Available
[ ] Observations/Notes on Respirator Condition
[ ] User Signature Verification

--- HEARING PROTECTION ---
[ ] Type of Hearing Protection Used (Earplugs (Disposable), Earplugs (Reusable), Earmuffs, Custom-Molded Earplugs)
[ ] Noise Level (dBA)
[ ] Condition of Earmuffs/Earplugs (Excellent, Good, Fair, Poor - Requires Replacement)
[ ] Last Replacement Date (Earplugs/Filters)
[ ] Notes/Comments on Hearing Protection

--- HIGH-VISIBILITY CLOTHING ---
[ ] High-Vis Vest Condition (Excellent, Good, Fair, Poor - Requires Replacement)
[ ] Reflective Tape Integrity (Intact & Bright, Slightly Damaged, Significantly Damaged/Faded)
[ ] Reflective Area (approximate %)
[ ] Visible Damage (Tears, Stains, Fading, Loose Stitching, None)
[ ] Last Garment Replacement Date

--- HAND PROTECTION (GLOVES) ---
[ ] Glove Type Selected (Cut Resistant, Chemical Resistant, Heat Resistant, General Purpose, Other)
[ ] Glove Thickness (mm)
[ ] Glove Size (S, M, L, XL, XXL)
[ ] Condition Notes (e.g., punctures, tears)
[ ] Date of Last Inspection

--- FOOT PROTECTION (SAFETY BOOTS) ---
[ ] Boot Type (Steel Toe, Composite Toe, ESD Safe, Waterproof)
[ ] Sole Thickness (mm)
[ ] Condition of Laces (Good, Fair, Damaged - Replace Required)
[ ] Condition of Upper (Good, Fair - minor wear, Damaged - Requires Repair/Replacement)
[ ] Notes (e.g., scuffs, tears)

--- BODY PROTECTION ---
[ ] Type of Body Protection Required (Coveralls, Flame-Resistant Clothing (FRC), High-Visibility Vest, Apron, None Required)
[ ] FRC Rating (If Applicable)
[ ] Last Inspection Date (Clothing)
[ ] Observed Defects (If Any)
[ ] Image of Clothing (if defects present)

--- TRAINING AND AWARENESS ---
[ ] Last PPE Training Date
[ ] Training Topics Covered (Hard Hat Usage, Eye Protection, Respiratory Protection, Hearing Protection, Gloves Selection, Foot Protection, General PPE Care & Maintenance)
[ ] Training Duration (Minutes)
[ ] Relevant Regulations Reviewed (Local Mining Regulations, National Safety Standards, Company PPE Policy, MSDS Sheets)
[ ] Employee Acknowledgement

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/mining-management/mining-ppe-compliance-checklist
(Click "Install Template" to launch your digital inspection tool immediately)