WAREHOUSE RACKING & STORAGE SAFETY INSPECTION CHECKLIST 2026
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--- STRUCTURAL INTEGRITY & FRAME INSPECTION ---
[ ] Upright Damage Severity (No Damage Detected, Minor Dent/Deformation, Significant Structural Damage, Critical/Immediate Repair Required)
[ ] Detailed Damage Description
[ ] Photo Documentation of Damage
[ ] Inspection Date
[ ] Inspector Verification

--- UPRIGHT & BASEPLATE STABILITY ---
[ ] Inspection Date
[ ] Aisle or Zone Number
[ ] Baseplate Condition (Secure & Intact, Loose or Damaged, Missing Bolts/Anchors)
[ ] Upright Verticality (Plumbness) (Within Tolerance, Visible Lean/Deformation)
[ ] Observations of Damage or Instability
[ ] Photo Documentation of Baseplate/Upright
[ ] Inspector Signature

--- BEAM & CONNECTION SECURITY ---
[ ] Safety Pin/Locking Clip Presence (All clips present and engaged, Missing or loose clips, Damaged or non-functional clips)
[ ] Beam Seating Condition (Securely seated, Dislodged/Improperly seated, Deformed/Bending)
[ ] Observed Beam Damage Details
[ ] Photo Evidence of Connection
[ ] Inspector Verification

--- LOAD CAPACITY & WEIGHT COMPLIANCE ---
[ ] Max Rated Capacity Verified (Yes, No, N/A)
[ ] Current Observed Load Weight (kg/lbs)
[ ] Load Distribution Status (Evenly Distributed, Uneven/Imbalanced, Overhanging)
[ ] Discrepancy Notes
[ ] Load Capacity Certificate/Manual Upload

--- PALLET & LOAD CONDITION ---
[ ] Pallet Condition Status (Good Condition, Damaged - Requires Replacement, Critical - Immediate Removal Required)
[ ] Identified Load Issues (Uneven Weight Distribution, Overhanging Goods, Obstructed View, Damaged Packaging, Improper Stacking Height)
[ ] Estimated Load Weight (kg/lbs)
[ ] Detailed Damage Description
[ ] Photo Documentation of Load/Pallet

--- AISLE CLEARANCE & FLOOR CONDITION ---
[ ] Aisle Obstruction Status (Clear, Obstructed, Partially Obstructed)
[ ] Description of Debris or Obstructions
[ ] Floor Surface Condition (Good Condition, Cracks Detected, Spills/Slippery Surface, Uneven/Potholes)
[ ] Photo of Floor/Aisle Condition
[ ] Inspection Date

--- SAFETY SIGNAGE & FLOOR MARKINGS ---
[ ] Pedestrian Walkway Visibility (Clear and highly visible, Faded or worn, Obstructed or missing)
[ ] Rack Load Capacity Signage Status (All signs present and legible, Missing or illegible signs, Signs damaged/unreadable)
[ ] Identified Safety Deficiencies (Missing floor tape, Unreadable warning signs, Obstructed emergency exits, Damaged bollard markings)
[ ] Detailed Observations
[ ] Photo Evidence of Markings
[ ] Inspection Date

--- PROTECTIVE GUARDING & BOLLARDS ---
[ ] Column Protector Condition (Intact, Damaged - Requires Repair, Missing/Destroyed)
[ ] Bollard Stability Assessment (Securely Anchored, Loose/Wobbling, Structural Damage Detected)
[ ] Damage Description
[ ] Photo Evidence of Damage
[ ] Date of Inspection
[ ] Inspector Signature

--- RACK HARDWARE & ACCESSORIES ---
[ ] Wire Decking Condition (Intact, Damaged/Bent, Missing, N/A)
[ ] Missing or Damaged Accessories (Safety Netting, Backstop Bars, Pallet Supports, Safety Pins/Clips)
[ ] Detailed Damage Description
[ ] Photo of Accessory Damage
[ ] Inspector Confirmation

--- INCIDENT REPORTING & MAINTENANCE LOG ---
[ ] Inspection Date
[ ] Warehouse Zone/Aisle Number
[ ] Incident Severity Level (Low (Minor cosmetic damage), Medium (Repair required soon), High (Immediate structural risk), Critical (Stop use/Evacuate area))
[ ] Description of Identified Damages or Incidents
[ ] Photos of Damaged Components
[ ] Corrective Action Plan
[ ] Inspector Signature
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