WAREHOUSE SAFETY AND FORKLIFT INSPECTION CHECKLIST TEMPLATE 2026

Created by ChecklistGuro (https://checklistguro.com)


--- PRE-SHIFT FORKLIFT INSPECTION (OPERATOR WALKAROUND) ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Forklift ID / Asset Number
[ ] Tire Condition (Good, Worn/Damaged, Needs Replacement)
[ ] Fork and Carriage Integrity (Pass, Fail)
[ ] Hydraulic Leak Detection (No Leaks Detected, Leak Detected)
[ ] Notes on Observed Damage or Wear
[ ] Upload Photo of Identified Issues
[ ] Operator Signature

--- OPERATIONAL SAFETY & CONTROL FUNCTIONALITY ---
[ ] Brake Functionality Check (Operational, Faulty, Not Applicable)
[ ] Steering and Directional Control (Smooth and Responsive, Sticky or Hard to Turn, Unresponsive)
[ ] Horn and Audible Alarm Status (Working, Not Working)
[ ] Hydraulic Lift and Tilt Operation (Smooth Operation, Leaking or Erratic Movement)
[ ] Warning Lights and Indicators Check (Headlights, Tail Lights, Blue Safety Spot Light, Dashboard Warning Indicators)
[ ] Reported Control Abnormalities
[ ] Operator Verification

--- BATTERY AND FUEL SYSTEM INSPECTION ---
[ ] Power Source Type (Electric (Battery), LPG (Propane), Diesel)
[ ] Battery Terminal Condition (Good/Clean, Corrosion Detected, Loose Connection, Needs Maintenance)
[ ] Fuel/Electrolyte Level Status (Sufficient, Low/Refill Required, Critical/Immediate Action Needed)
[ ] Leakage or Corrosion Details
[ ] Photo of Battery/Fuel Connection
[ ] Inspector Verification

--- WAREHOUSE FLOOR AND AISLEWAY SAFETY ---
[ ] Aisleway Obstruction Status (Clear and Accessible, Obstructed, Needs Immediate Action)
[ ] Identified Floor Hazards (Liquid Spills, Loose Debris/Trash, Damaged Floor Markings, Cracked/Uneven Concrete, Obstructed Pedestrian Lane)
[ ] Hazard Location Details
[ ] Corrective Actions Taken
[ ] Inspection Date
[ ] Inspector Verification

--- RACKING AND STORAGE INFRASTRUCTURE AUDIT ---
[ ] Rack Upright Condition (No visible damage, Minor dent/deformation, Critical structural damage)
[ ] Beam Connection Integrity (Secure and locked, Loose or misaligned, Missing safety clips)
[ ] Identified Hazards (Bent uprights, Obstructed aisles, Overloaded beams, Damaged pallet supports, Missing safety pins)
[ ] Damage Description and Remediation Plan
[ ] Photo Evidence of Damage
[ ] Inspection Date
[ ] Inspector Signature

--- PERSONAL PROTECTIVE EQUIPMENT (PPE) COMPLIANCE ---
[ ] PPE Items Verified (High-Visibility Vest, Steel-Toed Safety Boots, Hard Hat, Safety Glasses/Goggles, Work Gloves, Hearing Protection)
[ ] PPE Condition Assessment (All items in good condition, Some items require replacement, Critical PPE failure - Immediate action required)
[ ] PPE Deficiencies or Damage Details
[ ] Photo Evidence of Damaged PPE
[ ] Safety Officer Verification

--- EMERGENCY EQUIPMENT AND EXIT ACCESSIBILITY ---
[ ] Fire Extinguisher Inspection Status (Pass, Fail, Needs Service)
[ ] Emergency Exit Path Clearance (Clear, Obstructed)
[ ] Emergency Equipment Verified (First Aid Kit, Eye Wash Station, Fire Alarm System, Emergency Lighting, Spill Kits)
[ ] Deficiencies and Corrective Actions
[ ] Inspection Date
[ ] Inspector Signature

--- POST-SHIFT MAINTENANCE AND STORAGE PROTOCOL ---
[ ] Inspection Completion Date
[ ] Shift End Time
[ ] Forklift Parking Location (Charging Station A, Charging Station B, LPG Refueling Dock, Designated Maintenance Bay)
[ ] Post-Shift Cleaning Tasks Completed (Mast and Chains Cleaned, Debris Removed from Forks, Battery/Fuel Recharged, Controls Wiped Down)
[ ] Maintenance Issues or Incident Notes
[ ] Operator Signature

--- END OF TEMPLATE ---
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