WATER MANAGEMENT AND LEAK DETECTION PROCESS

Created by ChecklistGuro (https://checklistguro.com)

[ ] Fetch Sensor Data: Retrieve recent flow rate and pressure readings from the Water Meter Data Model.
[ ] Calculate Flow Variance: Compare current flow rate against the historical baseline to identify deviations.
[ ] Calculate Pressure Drop: Determine the difference between upstream and downstream pressure to detect potential leaks.
[ ] Aggregate Daily Consumption: Sum the total water volume recorded across all sensors for the last 24-hour period.
[ ] Threshold Comparison: Evaluate if the calculated variance or pressure drop exceeds the predefined safety thresholds.
[ ] Create Leak Incident Report: Generate a new entry in the 'Leak Incidents' data model when a threshold breach is detected.
[ ] Assign Field Technician: Create a task for the maintenance team to perform an on-site physical inspection.
[ ] Inspection Checklist: A set of steps for the technician to verify pipe integrity, valve status, and visible moisture.
[ ] Update Incident Status: Update the 'Leak Incident' entry status to 'Investigating' or 'Resolved' based on task completion.
[ ] Notify Operations Manager: Send an automated email alert to the Operations Manager regarding the detected anomaly.
[ ] Emergency SMS Alert: Send an urgent SMS to the on-call technician if a high-pressure burst is detected.
[ ] Fetch Asset Metadata: Retrieve pipe material and age information from the Asset Data Model to assess risk.
[ ] Weekly Water Loss Report: Generate a summary report of all detected leaks and repair costs for the weekly management review.
[ ] Cleanup False Alarms: Delete temporary anomaly entries that were flagged incorrectly by sensor noise.
[ ] Update Asset Maintenance Log: Update the 'Asset Data Model' to reflect the most recent repair date and maintenance notes.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/facility-management/water-management-and-leak-detection-process
(Click "Install Template" to launch your digital inspection tool immediately)