ACCESSIBILITY COMPLIANCE INSPECTION

Created by ChecklistGuro (https://checklistguro.com)

--- EXTERIOR ACCESS & CIRCULATION ---
[ ] Primary Entrance Location
[ ] Number of Designated Accessible Parking Spaces
[ ] Distance from Accessible Parking to Entrance (feet)
[ ] Accessible Parking Surface Condition (Stable and Level, Minor Cracks/Unevenness, Significant Damage/Unevenness - Potential Hazard)
[ ] Accessible Route to Entrance Type (Sidewalk, Ramp, Other (Specify))
[ ] Accessible Route Width (feet)
[ ] Obstacles on Accessible Route? (No, Yes (Specify in LONG_TEXT below))
[ ] Description of Obstacles (if any)
[ ] Photo of Accessible Route and Parking

--- ENTRANCES & DOORS ---
[ ] Minimum Clear Width at Entrance (inches)
[ ] Door Operating Force (lbs) (â‰¤ 5 lbs, â‰¤ 15 lbs (with power assist))
[ ] Door Swing Direction (Impact on Accessible Route) (Does not obstruct accessible route, Obstructs accessible route - mitigation required)
[ ] Clear Floor Space at Door (width in inches)
[ ] Clear Floor Space at Door (depth in inches)
[ ] Door Hardware Accessibility (Lever handles present, Hinges Accessible, Push/Pull Plates Present, Accessible Height, Other (specify in LONG_TEXT))
[ ] Additional Notes regarding hardware accessibility (if 'Other' selected)
[ ] Automatic Door Operation? (Yes, No)
[ ] Describe any observed issues with entrance/door accessibility

--- RAMPS & ELEVATORS ---
[ ] Ramp Slope (%)
[ ] Ramp Width (inches)
[ ] Landing Width at Bottom of Ramp (inches)
[ ] Landing Width at Top of Ramp (inches)
[ ] Ramp Handrails Present? (Yes, No, Not Applicable)
[ ] Elevator Presence? (Yes, No, Not Applicable)
[ ] Elevator Interior Width (inches)
[ ] Elevator Interior Depth (inches)
[ ] Elevator Control Panel Height (inches) (Less than 48 inches, Between 48 and 54 inches, Greater than 54 inches, N/A)
[ ] Any Elevator Maintenance/Repair Notes?

--- INTERIOR CIRCULATION & WAYFINDING ---
[ ] Minimum clear width of hallways (inches)
[ ] Turning radius at intersection of hallways (feet)
[ ] Are accessible routes clearly marked and free of obstructions? (Yes, No, N/A)
[ ] What types of obstructions are present on accessible routes? (Select all that apply) (Furniture, Storage, Debris, Construction Materials, None)
[ ] Describe any observed issues with accessible routes and provide suggestions for remediation.
[ ] Are tactile warning strips present at the edges of drop-offs? (Yes, No, N/A)
[ ] Describe signage and wayfinding clarity. Are signs at consistent heights and easily readable?
[ ] Are directional signage available and appropriately placed? (Yes, No, N/A)

--- RESTROOMS & HYGIENE FACILITIES ---
[ ] Toilet Stall Width (Minimum)
[ ] Clear Floor Space in Front of Toilet (Minimum Length)
[ ] Toilet Paper Dispenser Height (Above Finished Floor) (Less than 36 inches, 36-48 inches, Greater than 48 inches)
[ ] Grab Bar Presence & Placement (Check all that apply) (Toilet Adjacent Grab Bar Present (Left), Toilet Adjacent Grab Bar Present (Right), Grab Bar Height Correct (33-36 inches), Grab Bar Securely Mounted)
[ ] Sink Height (Above Finished Floor) (Less than 32 inches, 32-36 inches, Greater than 36 inches)
[ ] Notes on Sink Accessibility (e.g., knee clearance, insulation)
[ ] Accessible Toilet Paper Dispenser (Yes, No, N/A)
[ ] Mirror Accessibility (Check all that apply) (Mirror Edge No Closer than 27 inches to Floor, Clearance Provided Under Sink)

--- EMERGENCY EGRESS & SAFETY ---
[ ] Are accessible routes to all exits clearly marked and unobstructed? (Yes, No, N/A)
[ ] Number of accessible emergency exit signs present and functioning.
[ ] Are audible emergency alarms present and functioning? (Yes, No, N/A)
[ ] Are visual emergency alarms present and functioning? (Yes, No, N/A)
[ ] Describe any obstacles or conditions that hinder emergency egress for individuals with disabilities.
[ ] Are emergency exit routes wide enough to accommodate wheelchair users? (Yes, No, N/A)
[ ] Are fire extinguishers accessible and clearly visible? (Yes, No, N/A)
[ ] Date of last fire safety inspection.

--- COMMON AREAS & AMENITIES ---
[ ] Are accessible tables and seating available in the cafeteria/breakroom? (Yes, No, N/A - No Cafeteria/Breakroom)
[ ] Number of accessible seating options available in common waiting areas.
[ ] Which of the following amenities are provided in common areas? (Accessible vending machines, Accessible water fountains, Accessible ATMs, Accessible information kiosks, None)
[ ] Describe any observed barriers to accessibility within common areas (e.g., obstructions, inadequate space).
[ ] Are accessible routes clearly marked and maintained in common areas? (Yes, No, Partially)
[ ] Upload photos documenting accessibility of common areas.

--- MECHANICAL ROOMS & SERVICE AREAS (LIMITED ACCESS) ---
[ ] Accessible Route Presence?
[ ] Width of Accessible Route (feet)
[ ] Describe any obstacles or deviations from accessible route guidelines.
[ ] Presence of Accessible Electrical Panel? (Yes, No, N/A)
[ ] Are controls reachable without strain? (Yes, No, N/A)
[ ] Notes on accessibility of shut-off valves (if accessible).
[ ] Photo Documentation of Accessible Route/Conditions

--- GROUNDS MAINTENANCE & LANDSCAPE ---
[ ] Surface Slope (%)
[ ] Ground Cover Types Present (Paved Surface (Concrete, Asphalt), Gravel/Loose Stone, Grass/Turf, Mulch, Sand)
[ ] Ground Surface Stability (Stable and Firm, Slightly Uneven, Unstable/Loose)
[ ] Describe any observed obstructions (e.g., exposed tree roots, protruding rocks)
[ ] Width of Accessible Path (inches)
[ ] Obstacles present along accessible routes? (None, Shrubbery, Benches, Planters, Other (specify in LONG_TEXT))
[ ] Last Grounds Maintenance Date

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/facility-management/accessibility-compliance-inspection
(Click "Install Template" to launch your digital inspection tool immediately)