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--- PRE-OPERATIONAL SAFETY INSPECTION ---
[ ] Inspection Date
[ ] Safety Guard Status (All Guards Secure, Guards Missing/Damaged, Not Applicable)
[ ] Visual Leak Check Areas (Air Line Fittings, Pressure Relief Valves, Tank Drain Valves, Hose Couplings)
[ ] Current Ambient Temperature (°C/°F)
[ ] Inspector Signature

--- AIR COMPRESSOR UNIT INSPECTION ---
[ ] Drive Belt Condition (Good, Worn, Cracked/Damaged, Requires Immediate Replacement)
[ ] Oil Level Reading (Liters/Quarts)
[ ] Visual Inspection Checklist (No visible oil leaks detected, Motor mounting bolts are tight, Cooling fins are free of debris, No unusual vibration or noise)
[ ] Observations and Anomalies
[ ] Photo of Compressor Motor/Belts

--- PRESSURE VESSEL AND TANK INTEGRITY ---
[ ] Inspection Date
[ ] Tank Visual Condition (Good, Corroded, Dented/Damaged)
[ ] Current Tank Pressure (PSI)
[ ] Safety Valve Checkpoints (Relief Valve Operational, No Visible Leaks, No Corrosion Detected)
[ ] Notes on Tank Integrity Issues
[ ] Inspector Signature

--- AIR FILTRATION AND MOISTURE MANAGEMENT ---
[ ] Inspection Date
[ ] Air Filter Condition (Clean, Dirty - Needs Cleaning, Damaged - Requires Replacement)
[ ] Moisture Trap Drain Interval (Hours)
[ ] Maintenance Tasks Performed (Filter Element Replaced, Air Intake Cleaned, Condensate Drain Flushed, Moisture Separator Inspected)
[ ] Notes on Moisture or Debris Findings
[ ] Upload Photo of Filter/Separator Status
[ ] Technician Verification

--- PNEUMATIC TOOL & HOSE ASSESSMENT ---
[ ] Inspection Date
[ ] Hose Condition Status (Excellent, Good (Wear Detected), Critical (Requires Replacement))
[ ] Observed Issues (Cracks in Hose, Leaking Couplings, Damaged Tool Housing, Clogged Air Inlet)
[ ] Measured Operating Pressure (PSI)
[ ] Detailed Findings and Repair Notes
[ ] Technician Signature

--- REGULATOR AND GAUGE CALIBRATION ---
[ ] Calibration Date
[ ] Current Pressure Reading (PSI)
[ ] Regulator Functionality (Operational - Pressure Stabilized, Fluctuating - Requires Repair, Failed - Requires Immediate Replacement)
[ ] Gauge Deviation Notes
[ ] Technician Verification

--- LUBRICATION AND FLUID LEVELS ---
[ ] Date of Inspection
[ ] Oil Level Status (Adequate, Low - Refill Required, Critical - Immediate Action Needed)
[ ] Amount of Oil Added (Liters/Quarts)
[ ] Oil Type/Brand Used
[ ] Observations of Fluid Leaks or Contamination
[ ] Technician Signature

--- ELECTRICAL AND CONTROL SYSTEMS ---
[ ] Inspection Date
[ ] Control Panel Condition (Excellent, Good, Fair, Poor/Needs Repair)
[ ] Components Inspected (Pressure Switch, Emergency Stop Button, Wiring Harness, Circuit Breakers, Control Relays)
[ ] Electrical Faults or Observations
[ ] Technician Signature

--- POST-MAINTENANCE & CLEANUP ---
[ ] Cleanup Completion Notes
[ ] Completed Cleanup Tasks (Work area wiped down, Tools cleaned and stored, Spills cleaned/contained, Waste/Filters disposed of, Safety guards replaced)
[ ] Completion Date
[ ] Technician Signature
[ ] Post-Maintenance Photo
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