AS-BUILT DRAWINGS VERIFICATION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- DOCUMENT REVIEW & INITIAL ASSESSMENT ---
[ ] Drawing Set Number/Version
[ ] Date of Initial Review
[ ] Overall Impressions/Preliminary Observations
[ ] Completeness of Drawing Set (Complete, Mostly Complete, Incomplete)
[ ] Preliminary Discrepancies Identified (if any)
[ ] Attach Initial Drawing Set (PDF)
[ ] Drawing Legend & Symbols Clear? (Yes, No, Unclear)

--- STRUCTURAL ELEMENTS VERIFICATION ---
[ ] Foundation Elevation - As-Built vs. Original
[ ] Column Spacing - As-Built vs. Design
[ ] Notes/Observations Regarding Foundation Construction
[ ] Beam Size Verification (Correct, Incorrect - Requires Revision, Not Found/Missing)
[ ] Location of Discrepancy (if any)
[ ] Photos/Documentation of Discrepancies (if any)
[ ] Slab Thickness - As-Built vs. Design
[ ] Wall Alignment Verification (Correct, Incorrect - Requires Revision, Not Found/Missing)

--- MECHANICAL, ELECTRICAL, AND PLUMBING (MEP) SYSTEMS VERIFICATION ---
[ ] HVAC Ductwork Routing Accurate? (Yes, No, Not Verified)
[ ] Piping Layout Matches Drawings? (Yes, No, Not Verified)
[ ] Electrical Conduit Size Verification (Diameter in inches)
[ ] Notes on Electrical Panel Locations
[ ] Photo of Plumbing Penetrations
[ ] Equipment Locations Verified? (Yes, No, Not Verified)
[ ] Comments on any Fire Protection System Deviations

--- ARCHITECTURAL FEATURES VERIFICATION ---
[ ] Verify Window Locations (Match As-Built, Discrepancy Found - Documented)
[ ] Verify Door Locations (Match As-Built, Discrepancy Found - Documented)
[ ] Describe any discrepancies in Finish Schedules (e.g., flooring, wall coverings)
[ ] Upload photos of discrepancies in architectural details (if any)
[ ] Verify Location of Architectural Blockouts/Openings (Match As-Built, Discrepancy Found - Documented)
[ ] If finish material differs, record the square footage discrepancy (if applicable)
[ ] Note any differences in architectural trim details (crown molding, baseboards, etc.)

--- SITE IMPROVEMENTS & EXTERIOR WORKS VERIFICATION ---
[ ] Verify Site Grading & Topography Matches As-Built
[ ] Confirm Pavement Types and Locations (Asphalt, Concrete, Gravel, Other (Specify in LONG_TEXT))
[ ] Detailed Notes on Landscaping Verification (Species, Locations, etc.)
[ ] Distance from Building to Nearest Utility Connection (Feet)
[ ] Photos of Exterior Features & Site Improvements (for comparison)
[ ] Confirm Utility Connection Points (Match As-Built?) (Match, Discrepancy - Detail in LONG_TEXT)
[ ] Describe Any Discrepancies Found in Exterior Lighting Layout

--- RECORD KEEPING & DOCUMENTATION ---
[ ] Summary of Discrepancies Found
[ ] Detailed Description of Each Discrepancy (Include Location, Drawing Number, etc.)
[ ] Total Number of Discrepancies Identified
[ ] Supporting Photographs/Documentation of Discrepancies
[ ] Discrepancy Resolution Status (Open, Resolved, Pending Review, Rejected)
[ ] Date Discrepancy Reported
[ ] Date Discrepancy Resolved (if applicable)
[ ] Resolution Description (How discrepancy was resolved)
[ ] Reviewer Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/as-built-drawings-verification-checklist
(Click "Install Template" to launch your digital inspection tool immediately)