ASSEMBLY LINE ERGONOMICS CHECKLIST: MANUFACTURING WORKPLACE HEALTH & SAFETY PRACTICES

Created by ChecklistGuro (https://checklistguro.com)

--- WORKSTATION LAYOUT & DESIGN ---
[ ] Work Surface Height (inches)
[ ] Distance to Nearest Frequently Used Tool (inches)
[ ] Work Surface Material (Wood, Metal, Anti-Fatigue Mat, Other)
[ ] Reach Distance Assessment (Optimal, Requires Adjustment, Excessive Reach)
[ ] Notes on Workstation Layout
[ ] Workstation Coordinates

--- TOOL AND EQUIPMENT ASSESSMENT ---
[ ] Tool Weight Adjustment (Appropriate, Too Heavy, Too Light)
[ ] Handle Diameter (mm)
[ ] Tool Grip Comfort (Comfortable, Somewhat Comfortable, Uncomfortable)
[ ] Describe any difficulties encountered using the tool.
[ ] Upload photo of tool/equipment.
[ ] Equipment Vibration Level (Acceptable, Noticeable, Excessive)

--- MATERIAL HANDLING PROCEDURES ---
[ ] Average Lift Weight (lbs)
[ ] Frequency of Lifting (lifts/hour)
[ ] Lifting Method (Manual, Assisted, Automated) (Manual, Assisted (e.g., hoist), Automated (e.g., conveyor))
[ ] Handling Aids Used (Check all that apply) (Hand Trucks, Pallet Jacks, Forklifts, Hoists, Dollies, None)
[ ] Describe Material Handling Procedure
[ ] Employee Training Status (Trained, Not Trained)

--- WORKER POSTURE AND BODY MECHANICS ---
[ ] Reach Distance (inches)
[ ] Typical Body Posture Observed (select one) (Upright, Forward Lean, Bending, Twisting, Awkward Position)
[ ] Describe any unusual body movements observed.
[ ] Level of Trunk Bending (select one) (Minimal, Moderate, Significant)
[ ] Frequency of Repetitive Bending/Twisting (times/minute)
[ ] Notes on worker comfort levels (verbal feedback)

--- REPETITIVE MOTION ANALYSIS ---
[ ] Estimated Cycles Per Hour
[ ] Primary Motion Type (e.g., Wrist Flexion, Shoulder Rotation) (Wrist Flexion/Extension, Shoulder Rotation, Elbow Flexion/Extension, Finger/Thumb Movements, Other (Specify in Long Text))
[ ] Description of Repetitive Motion (if 'Other' selected above)
[ ] Average Duration of Repetitive Motion Cycle (seconds)
[ ] Potential Risk Factors Observed (Check all that apply) (Awkward Posture, Excessive Force, High Repetition Rate, Lack of Breaks, Insufficient Training)
[ ] Worker Comments/Concerns Regarding Repetitive Motion
[ ] Immediate Action Required (if any) (None, Adjust Workstation Height, Modify Task Sequence, Provide Assistive Device, Provide Additional Training)

--- LIGHTING AND VISIBILITY ---
[ ] Ambient Light Level (Lux)
[ ] Light Source Type (LED, Fluorescent, Incandescent, Natural, Other)
[ ] Visibility Issues Observed (Glare, Shadows, Reflections, Insufficient Illumination, None)
[ ] Specific Areas with Poor Visibility
[ ] Date of Last Lighting Inspection

--- TRAINING AND EDUCATION ---
[ ] Training Module Completion (Ergonomics 101) (Completed, In Progress, Not Started)
[ ] Date of Last Ergonomics Training
[ ] Hours of Ergonomics Training Received (Total)
[ ] Supervisor Confirmation of Training Adequacy (Yes, No)
[ ] Notes on Employee Understanding of Ergonomic Principles

--- PERSONAL PROTECTIVE EQUIPMENT (PPE) ---
[ ] Required PPE for Task (Safety Glasses, Gloves, Hearing Protection, Respirator, Safety Shoes, Face Shield, Apron)
[ ] Condition of Safety Shoes (1-10, 10=Excellent)
[ ] Glove Type (Nitrile, Latex, Leather, Cut-Resistant)
[ ] Respirator Fit Test Date (if applicable)
[ ] Last Inspection Date of Safety Glasses

--- FEEDBACK AND CONTINUOUS IMPROVEMENT ---
[ ] Worker Suggestions for Ergonomic Improvements
[ ] Number of Ergonomic Issues Reported This Period
[ ] Were Workers Satisfied with Recent Ergonomic Adjustments? (Yes, No, Neutral)
[ ] Date of Last Ergonomics Review Meeting
[ ] Which areas require further investigation based on feedback? (Workstation Layout, Tooling, Material Handling, Training)
[ ] Summary of Action Items from Review Meeting

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/manufacturing/assembly-line-ergonomics-checklist-manufacturing-workplace-health-safety-practices
(Click "Install Template" to launch your digital inspection tool immediately)