AUTOMATED PIT SLOPE STABILITY MONITORING

Created by ChecklistGuro (https://checklistguro.com)

[ ] Fetch Sensor Readings: Retrieve the latest displacement and pore pressure readings from the Pit Slope Sensor data model.
[ ] Retrieve Threshold Limits: Fetch the predefined safety threshold values (Alert and Alarm levels) from the Site Safety Configuration model.
[ ] Calculate Velocity of Movement: Calculate the rate of change in displacement by comparing the current reading to the previous reading.
[ ] Calculate Factor of Safety (FoS): Execute a formula using pore pressure and displacement data to estimate the current stability ratio.
[ ] Determine Alert Status: Compare calculated velocity and FoS against the retrieved threshold limits to determine status (Green, Yellow, Red).
[ ] Average Daily Movement: Calculate the average displacement across all sensors in a specific pit sector over the last 24 hours.
[ ] Update Sensor Status: Update the 'Last Checked' timestamp and 'Current Health' status in the Sensor data model.
[ ] Trigger Visual Inspection Task: Create a high-priority task for the Geotechnical Engineer if movement exceeds the 'Alert' threshold.
[ ] Create Maintenance Work Order: Create a task for the Maintenance Team if a sensor reports a low battery or hardware error.
[ ] Notify Site Manager (Alert): Send an email notification to the Site Manager containing the summarized stability report when thresholds are breached.
[ ] Emergency SMS Alert: Send an urgent SMS to the Pit Supervisor and Safety Officer if the 'Alarm' (Red) threshold is triggered.
[ ] Log Incident Report: Create a new entry in the Incident Log data model whenever a threshold breach occurs.
[ ] Generate Daily Stability Report: Generate a PDF summary report of all sensor trends and stability metrics for the previous 24-hour period.
[ ] Clear Resolved Alerts: Delete transient alert notifications from the active 'Active Alerts' data model once the stability issue is resolved.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/mining-management/automated-pit-slope-stability-monitoring
(Click "Install Template" to launch your digital inspection tool immediately)