AUTOMOTIVE ELECTRIC VEHICLE (EV) CHARGING STATION MAINTENANCE CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- VISUAL INSPECTION ---
[ ] Station ID
[ ] Ambient Temperature (°C)
[ ] Overall Condition (Excellent, Good, Fair, Poor)
[ ] Describe Any Visible Damage
[ ] Evidence of Vandalism? (Yes, No)
[ ] Upload Photo of Station

--- CABLE AND CONNECTOR ASSESSMENT ---
[ ] Cable Condition (Excellent, Good, Fair, Poor)
[ ] Connector Pins Condition (Clean, Slight Corrosion, Moderate Corrosion, Significant Corrosion)
[ ] Cable Fraying Length (mm)
[ ] Connector Pin Bending (mm)
[ ] Additional Notes
[ ] Photos of Damage

--- DISPLAY AND INTERFACE FUNCTIONALITY ---
[ ] Display Readability (Brightness, Contrast)
[ ] Error Messages Displayed? (Yes, No)
[ ] Description of any displayed error messages
[ ] Brightness Level (if adjustable)
[ ] User Interface Responsiveness (Very Responsive, Responsive, Slightly Lagging, Lagging)
[ ] Last Firmware Update Date

--- CHARGING PORT INTEGRITY ---
[ ] Describe any visible damage to the charging port (scratches, cracks, etc.)
[ ] Connector Pin Corrosion Level (0-5, 0=None, 5=Severe)
[ ] Connector Type (Type 1 (CHAdeMO), Type 1 (J1772), Type 2 (Mennekes), CCS Combo 1, CCS Combo 2, Tesla Proprietary)
[ ] Connector Pin Resistance (Ohms)
[ ] Record any unusual sounds or smells detected at the charging port.
[ ] Connector Condition (Excellent, Good, Fair, Poor)

--- SAFETY FEATURES VERIFICATION ---
[ ] Technician Signature (Emergency Stop Test)
[ ] Emergency Stop Activation Time (seconds)
[ ] Emergency Stop Button Status (Functional, Needs Repair)
[ ] Emergency Stop Button Press Count (for functionality test)
[ ] Power Interlock Functionality Check (Pass, Fail)

--- SOFTWARE AND FIRMWARE UPDATES ---
[ ] Last Update Date
[ ] Current Firmware Version
[ ] Update Method (Automatic, Manual, Network Push)
[ ] Update Notes
[ ] Success Status (Successful, Partial Success, Failed)

--- POWER SUPPLY AND CONNECTIONS ---
[ ] Input Voltage (V)
[ ] Output Voltage (V)
[ ] Input Current (A)
[ ] Output Current (A)
[ ] Connection Type (Hardwired, Plug-in)
[ ] Connection Status (Secure, Loose, Corroded)
[ ] Notes on Connection Integrity

--- ENVIRONMENTAL FACTORS ---
[ ] Ambient Temperature (°C)
[ ] Relative Humidity (%)
[ ] Exposure to Direct Sunlight (No, Minimal, Moderate, Significant)
[ ] Evidence of Precipitation/Moisture (No, Minor, Moderate, Significant)
[ ] Last Snow/Ice Event

--- REPORTING & DOCUMENTATION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Temperature (°C)
[ ] Detailed Observations/Notes
[ ] Overall Condition (Excellent, Good, Fair, Poor)
[ ] Inspector Signature
[ ] Supporting Photos (Optional)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/automotive/automotive-electric-vehicle-ev-charging-station-maintenance-checklist
(Click "Install Template" to launch your digital inspection tool immediately)