BELT TENSION AND ALIGNMENT

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-INSPECTION & SAFETY ---
[ ] Confirm Lockout/Tagout Procedures? (Yes, No, N/A)
[ ] Personal Protective Equipment (PPE) Verified? (Yes, No)
[ ] Brief description of equipment being inspected:
[ ] Date of Last Inspection
[ ] Equipment ID Number
[ ] Environment (Indoor/Outdoor) (Indoor, Outdoor)

--- BELT VISUAL INSPECTION ---
[ ] Describe any visible belt damage (cracks, fraying, cuts, missing chunks)
[ ] Identify belt wear patterns: (Even wear, Edge wear, Center wear, Spot wear, None observed)
[ ] Estimate the percentage of belt surface area affected by wear.
[ ] Belt Contamination Status: (Clean, Minor Contamination, Significant Contamination (Oil, Debris))
[ ] Upload a photograph of the belt condition (optional)
[ ] Note any unusual noises during belt rotation (e.g., squealing, chirping)

--- BELT TENSION MEASUREMENT ---
[ ] Belt Tension Reading (lbs/in)
[ ] Belt Tension Measurement Tool Used (Calibration Date)
[ ] Tension Measurement Method (Dial Indicator, Tension Gauge, Ruler/Marking Method, Other (Specify))
[ ] Notes on Tension Reading (e.g., inconsistent readings, unusual behavior)
[ ] Tension Within Specified Range? (Yes, No, N/A - No Specified Range)

--- BELT ALIGNMENT VERIFICATION ---
[ ] Pulley Parallelism (Side View)
[ ] Pulley Parallelism (Top View)
[ ] Belt Tracking (Left/Right) (Left, Right, Centered)
[ ] Pulley Face Condition (Clean, Slightly Dirty, Dirty/Rough)
[ ] Notes on Alignment Issues
[ ] Measurement of Pulley Offset (if applicable)

--- ADJUSTMENT & CORRECTION ---
[ ] New Belt Tension (lbs/inch)
[ ] Adjustment Increment (lbs/inch)
[ ] Adjustment Method (Take-up Idler, Adjustable Pulley, Belt Stretchers, Other (Specify Below))
[ ] If 'Other' Adjustment Method, please specify:
[ ] Alignment Correction Method (Shim Adjustment, Pulley Repositioning, Belt Re-Routing, Other (Specify Below))
[ ] If 'Other' Alignment Correction Method, please specify:
[ ] Alignment Adjustment Amount (inches)
[ ] Belt Type (V-belt, Ribbed Belt, Flat Belt, Timing Belt)

--- POST-ADJUSTMENT VERIFICATION ---
[ ] Re-measured Belt Tension (after adjustment)
[ ] Belt Noise Level (after adjustment) (None, Slight, Moderate, Loud)
[ ] Drive Stability During Operation (Stable, Minor Vibration, Significant Vibration, Slippage)
[ ] Pulley RPM (if applicable)
[ ] Any Unusual Observations During Operation (e.g., excessive heat, unusual sounds)
[ ] Belt Condition Post Adjustment (Improved, No Change, Worse)

--- DOCUMENTATION & RECORD KEEPING ---
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Belt Tension Reading (Initial)
[ ] Belt Tension Reading (Final)
[ ] Observations and Notes (e.g., specific belt condition, unusual noises)
[ ] Belt Type (V-Belt, Flat Belt, Ribbed Belt, Other)
[ ] Equipment/Machine ID
[ ] Corrective Actions Taken
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/agriculture/belt-tension-and-alignment
(Click "Install Template" to launch your digital inspection tool immediately)