BUS STOP ACCESSIBILITY COMPLIANCE INSPECTION CHECKLIST - PUBLIC TRANSIT

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL INFORMATION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Bus Stop Location (GPS Coordinates)
[ ] Bus Stop ID (Enter Bus Stop ID)
[ ] Inspector Name
[ ] Inspector Role (Accessibility Auditor, Transit Planner, Maintenance Staff)
[ ] Weather Conditions

--- PHYSICAL ACCESSIBILITY - PATH OF TRAVEL ---
[ ] Start Point of Path of Travel
[ ] Path Width (feet)
[ ] Surface Material (Concrete, Asphalt, Gravel, Other)
[ ] Path Slope (%) (0-2%, 2-5%, 5% or greater)
[ ] Obstacles Present? (Overhanging Branches, Parked Vehicles, Signage, Utility Covers, None)
[ ] Description of Obstacles (if any)
[ ] Path Condition (Excellent, Good, Fair, Poor)

--- BUS STOP PLATFORM ACCESSIBILITY ---
[ ] Platform Height (inches)
[ ] Platform Levelness (Level, Slightly Sloped, Significantly Sloped)
[ ] Platform Surface Material (Concrete, Asphalt, Paved, Other)
[ ] Presence of Raised Edges (Yes, No, Partial)
[ ] Width of Platform (feet)
[ ] Notes on Platform Condition
[ ] Tactile Warning Surface Present? (Yes, No)

--- BUS STOP SHELTER ACCESSIBILITY ---
[ ] Shelter Width (feet)
[ ] Shelter Depth (feet)
[ ] Ramp Presence (Yes, No, N/A)
[ ] Door Width (minimum 32 inches) (Yes, No, N/A)
[ ] Accessible Seating Features (Backless Seating, Armrests, Sufficient Space for Mobility Devices, N/A)
[ ] Shelter Lighting Adequate? (Yes, No, N/A)
[ ] Additional Notes on Shelter Accessibility

--- SIGNAGE & INFORMATION ACCESSIBILITY ---
[ ] Signage Legibility - Overall Assessment (Excellent, Good, Fair, Poor)
[ ] Tactile Information Present on Signage? (Yes, No, Not Applicable)
[ ] Font Size (in points)
[ ] Contrast Ratio - Text to Background (Meets Standard, Does Not Meet Standard, Not Applicable)
[ ] Comments on Signage Content
[ ] Signage Height - Position relative to street level (Optimal, Too High, Too Low, Not Applicable)

--- CURBING & CROSSING ACCESSIBILITY ---
[ ] Curb Ramp Location (GPS Coordinates)
[ ] Curb Ramp Slope (%)
[ ] Curb Ramp Tactile Indicators Present? (Yes, No, Not Applicable)
[ ] Curb Ramp Surface Condition? (Excellent, Good, Fair, Poor)
[ ] Pedestrian Signal Accessible Button Present? (Yes, No, Not Applicable)
[ ] Signal Timing for Accessible Crossing (seconds)
[ ] Description of Crossing Environment (traffic volume, visibility)

--- LIGHTING & VISIBILITY ---
[ ] Ambient Light Level (Lux)
[ ] Adequacy of General Lighting (Sufficient, Marginal, Insufficient)
[ ] Presence of Glare? (Yes, No)
[ ] Description of Lighting Conditions (if applicable)
[ ] Presence of Obstructions to Light? (Yes, No)
[ ] Distance to Nearest Light Source (meters)

--- OBSTACLES & CLEARANCES ---
[ ] Clearance from Obstacles (inches)
[ ] Width of Accessible Path (inches)
[ ] Overhanging Branches/Obstructions? (Yes, No)
[ ] Identify any obstructions (check all that apply) (Trash Cans, Street Furniture, Utility Poles, Vegetation, Other)
[ ] Describe any observed obstructions in detail
[ ] Is there sufficient clearance for mobility devices? (Yes, No)
[ ] Location of Obstruction (if applicable)

--- SUMMARY & RECOMMENDATIONS ---
[ ] Overall Summary of Accessibility Compliance
[ ] Severity Rating (1-5, 1=Minor, 5=Critical)
[ ] Areas Requiring Immediate Action (Platform Surface, Curb Ramp, Shelter Accessibility, Signage, Path of Travel, Other)
[ ] Specific Recommendations for Improvement
[ ] Date of Next Review
[ ] Inspector Signature
[ ] GPS Location of Inspection

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/bus-stop-accessibility-compliance-inspection-checklist-public-transit
(Click "Install Template" to launch your digital inspection tool immediately)