CONSTRUCTION SITE SAFETY INSPECTION CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- SITE ACCESS & SECURITY ---
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Main Site Access Point
[ ] Perimeter Fencing Condition (Excellent, Good, Fair, Poor)
[ ] Access Points Secured? (Main Gate, Secondary Gate, Service Entrance, Perimeter Fence Breaches)
[ ] Visitor Log Maintained? (Yes, No)
[ ] Visitor Signature Verification

--- PERSONAL PROTECTIVE EQUIPMENT (PPE) ---
[ ] Hard Hats Being Worn? (Yes, No, N/A)
[ ] Safety Glasses/Face Shields Being Worn? (Yes, No, N/A)
[ ] Number of Employees Observed Without Required PPE
[ ] Gloves Being Worn (Type Appropriate for Task?) (Yes, No, N/A)
[ ] Foot Protection (Steel-toed boots etc.) (Compliant, Non-Compliant, N/A)
[ ] PPE Issues / Corrective Actions Required

--- EXCAVATION & TRENCHING ---
[ ] Excavation Depth (ft)
[ ] Trench Shoring Method (Shoring, Sloping, Benching, No System Required (<= 5ft))
[ ] Soil Type (for Sloping/Benching) (Type 1, Type 2, Type 3, Type 4)
[ ] Maximum Slope Angle (degrees)
[ ] Underground Utility Location Verified? (Yes - Marked on Surface, Yes - Contacted Utility Company, No - Unknown, No - Not Applicable)
[ ] Utility Company Contacted (if applicable)
[ ] Date of Utility Location Verification
[ ] Describe any observed hazards or deficiencies

--- FALL PROTECTION ---
[ ] Height of Work Area (feet)
[ ] Type of Fall Protection Used (Guardrail, Personal Fall Arrest System (PFAS), Safety Net, Controlled Access Zone, Other (Specify in Long Text))
[ ] If 'Other' selected above, please specify:
[ ] Guardrail Condition (Excellent, Good, Fair, Poor - Requires Repair)
[ ] PFAS Inspection Points (Check all that apply) (Harness Condition, Lanyard Condition, Anchor Point Integrity, Proper Fit & Adjustment, Connection Points Secure)
[ ] Last PFAS Inspection Date
[ ] Inspector Signature

--- ELECTRICAL SAFETY ---
[ ] Voltage of Temporary Power Source (V)
[ ] Grounding System Status (Adequate, Inadequate, N/A)
[ ] Electrical Hazards Observed (Exposed Wiring, Damaged Insulation, Overloaded Circuits, Missing Grounding, None)
[ ] Details of Electrical Hazards Found
[ ] Date of Last Electrical Equipment Inspection
[ ] Condition of Extension Cords (Good, Damaged, N/A)

--- SCAFFOLDING & LADDERS ---
[ ] Scaffold Height (feet)
[ ] Scaffold Base Condition (Stable & Level, Unstable, Slightly Unstable)
[ ] Guardrail Condition (Present, Missing, Damaged, Proper Height, Secure)
[ ] Ladder Type (Step Ladder, Extension Ladder, Fixed Ladder)
[ ] Ladder Angle (degrees)
[ ] Ladder Extension Above Landing (3 feet, Less than 3 feet, N/A)
[ ] Ladder Condition Notes (Rungs, Steps, Rails)

--- HEAVY EQUIPMENT & MACHINERY ---
[ ] Equipment Hour Meter Reading
[ ] Fluid Levels (Oil, Coolant, Hydraulic) (Normal, Low, High, Requires Attention)
[ ] Tire Condition (if applicable) (Good, Fair, Poor - Requires Replacement, N/A)
[ ] Brake System Check (Functional, Noisy, Leaking, Requires Attention)
[ ] Any Unusual Noises or Vibrations?
[ ] Load Capacity (Max Allowed)
[ ] Safety Guards in Place? (Yes, No, N/A)
[ ] Last Maintenance Date

--- HAZARD COMMUNICATION ---
[ ] Number of Safety Data Sheets (SDS) Available
[ ] SDS Locations Verified (Check all that apply) (Main Office, Tool Crib, Jobsite Trailer, Vehicle Storage, Other (Specify))
[ ] If 'Other' Selected Above, Please Specify Location:
[ ] SDS Training Last Conducted (Select Date)
[ ] Date of Last Hazard Communication Training
[ ] Summary of Hazard Communication Training Content
[ ] Attach SDS Training Roster
[ ] Container Labeling Compliance: Are chemical containers properly labeled? (Yes, No, N/A)

--- HOUSEKEEPING ---
[ ] Debris Volume (Cubic Yards)
[ ] Identify Trip Hazards Present? (Loose Materials, Uneven Surfaces, Hoses/Cords, Tools/Equipment Left Out, None)
[ ] Description of Housekeeping Issues Observed
[ ] Condition of Walkways/Access Routes? (Clear & Safe, Slight Obstructions, Significant Obstructions, Unsafe)
[ ] Number of Unsecured Tools/Materials
[ ] Notes on Waste Management Practices

--- FIRE PREVENTION & PROTECTION ---
[ ] Fire Extinguisher Inspection Date
[ ] Fire Extinguisher Condition (Visual) (Good, Damaged, Missing, Obstructed)
[ ] Fire Lane Clearance (Clear, Obstructed, Partially Obstructed)
[ ] Last Fire Drill Date
[ ] Sprinkler System Inspection Status (Inspected and Operational, Needs Inspection, Out of Service)
[ ] Comments/Observations (Fire Prevention & Protection)

--- CONFINED SPACE ENTRY ---
[ ] Permit Issue Date
[ ] Entry Start Time
[ ] Permit Status (Active, Inactive, Cancelled)
[ ] Hazards Identified (Oxygen Deficiency, Toxic Gases, Flammable Atmosphere, Engulfment Hazards, Other)
[ ] Detailed Hazard Description
[ ] Entry Supervisor (Name 1, Name 2, Name 1)
[ ] Oxygen Level (%)
[ ] Lethane Level (ppm)

--- ENVIRONMENTAL COMPLIANCE ---
[ ] Rainfall Amount (mm) - Recent Precipitation
[ ] Erosion Control Measures in Place? (Yes, No, Partially Implemented)
[ ] Describe any observed erosion issues:
[ ] Photo Documentation of Erosion Control (if needed)
[ ] Waste Management Plan Followed? (Yes, No, N/A)
[ ] Amount of Waste Generated (estimated cubic meters)
[ ] Date of Last Spill Prevention Plan Review
[ ] Describe any observed environmental concerns or spills:

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/inspection-management/construction-site-safety-inspection-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)