DAILY HVAC SYSTEM CHECK

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL VISUAL INSPECTION ---
[ ] Overall System Appearance
[ ] Ambient Temperature (Outdoor)
[ ] Ambient Temperature (Indoor)
[ ] Unusual Noises Detected? (No, Yes - Describe in Long Text)
[ ] Describe any unusual noises or observations (if applicable)
[ ] Signs of Leaks (Water/Refrigerant)? (No, Yes - Specify Location)
[ ] Specify location of any leaks (if applicable)
[ ] Evidence of Pests/Rodents? (No, Yes - Document with File Upload)
[ ] Evidence of Pests/Rodents (if applicable)

--- OUTDOOR UNIT(S) - CONDENSERS ---
[ ] Ambient Temperature (°F/°C)
[ ] Suction Line Pressure (PSI/kPa)
[ ] Discharge Line Pressure (PSI/kPa)
[ ] Fan Operation (Normal, Noisy, Not Operating)
[ ] Coil Condition (Clean, Slightly Dirty, Dirty, Very Dirty)
[ ] Debris Around Unit (Leaves, Grass, Branches, Other)
[ ] Notes/Observations

--- INDOOR UNIT(S) - AIR HANDLING UNITS (AHUS) ---
[ ] Supply Air Temperature (degrees F)
[ ] Return Air Temperature (degrees F)
[ ] AHU Static Pressure (inches of water)
[ ] Fan Operation (Normal, Humming, Clicking, Stopped)
[ ] Coil Condition (Visual) (Clean, Slightly Dirty, Dirty, Excessively Dirty)
[ ] Notes on Coil Condition
[ ] Condensate Drain Status (Free Flowing, Slow Flow, Blocked)
[ ] Description of any unusual noises

--- CHILLER/BOILER (IF APPLICABLE) ---
[ ] Chiller/Boiler Inlet Water Temperature (°F)
[ ] Chiller/Boiler Outlet Water Temperature (°F)
[ ] Condenser Water Pressure (PSI)
[ ] Boiler Pressure (PSI) - if applicable
[ ] Burner Operation (if applicable) (Normal, Flashing, Off, Other)
[ ] Vibration Level (Normal, Slight, Moderate, Severe)
[ ] Notes/Observations (e.g., unusual noises, leaks, error codes)

--- DUCTWORK & AIRFLOW ---
[ ] Airflow from Supply Registers (General) (Adequate, Weak, Excessive, Restricted)
[ ] Static Pressure (if monitored - in inches of water)
[ ] Ductwork Condition (Visible Sections) (Good, Minor Damage, Significant Damage, Leaking/Loose)
[ ] Notes on Ductwork/Airflow Concerns
[ ] Return Airflow Condition (Normal, Restricted, Excessive)
[ ] Location of Identified Ductwork Issues

--- ZONE CONTROL & THERMOSTATS ---
[ ] Thermostat Setting (Room 101)
[ ] Thermostat Functionality (Room 205) (Working Correctly, Not Responding, Erratic Readings, Display Malfunction)
[ ] Zone Damper Operation (Zone A) (Opening as Expected, Stuck Closed, Stuck Open, Noisy Operation)
[ ] Room Temperature (Suite 302)
[ ] Notes on Zone Control Issues
[ ] Thermostat Calibration Required? (Yes, No)

--- CONDENSATE MANAGEMENT ---
[ ] Describe Condensate Drain Condition
[ ] Measure Condensate Pan Water Level (inches)
[ ] Drain Flow Appearance (Clear, Slightly Cloudy, Cloudy/Murky, Visible Debris)
[ ] Drain Line Obstruction Present? (Yes, No)
[ ] If Yes to Obstruction, describe obstruction details and action taken
[ ] Measure Condensate Pump Discharge Pressure (PSI)
[ ] Condensate Pump Operating Noise (Normal, Loud, Humming, Rattling)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/hospitality/daily-hvac-system-check
(Click "Install Template" to launch your digital inspection tool immediately)