DAILY WAREHOUSE WALKTHROUGH INSPECTION

Created by ChecklistGuro (https://checklistguro.com)

--- SAFETY & HAZARDS ---
[ ] Are there any visible hazards present (e.g., spills, obstructions)? (Yes - Spill, Yes - Obstruction, Yes - Trip Hazard, Yes - Other (Specify in LONG_TEXT), No)
[ ] If 'Yes' was selected above, please describe the hazard(s) in detail.
[ ] Ambient Temperature (Celsius/Fahrenheit - specify in LONG_TEXT)
[ ] Note any unusual smells or signs of potential fire hazards.
[ ] Are fire extinguishers easily accessible and appear to be in good working order? (Yes, No - Blocked, No - Appears damaged)
[ ] PPE Compliance - Observed any issues with employee use of appropriate PPE (e.g., hard hats, safety shoes)? (No issues observed, Missing Hard Hats, Incorrect Footwear, No Gloves, Other (Specify in LONG_TEXT))
[ ] Any additional safety concerns or observations?

--- DOCK AREA & RECEIVING ---
[ ] Dock Door Condition (Scale 1-5, 1=Poor, 5=Excellent)
[ ] Dock Leveler Functionality (Functional, Needs Repair, Out of Service)
[ ] Receiving Area Issues? (Overcrowding, Damage to Goods, Incorrect Palletizing, Lack of Space, None)
[ ] Notes on Pallet Condition (Quality, Damage)
[ ] Temperature of Receiving Area (if applicable)
[ ] Number of Damaged Pallets Received

--- STORAGE RACKING & LAYOUT ---
[ ] Racking Condition - Visual Inspection (No Damage Observed, Minor Scratches/Wear, Bent Uprights, Missing Hardware (bolts, clips), Damaged Beams, Significant Rust/Corrosion)
[ ] Rack Spacing - Minimum Clearance (inches)
[ ] Aisle Markings & Visibility (Clearly Marked and Visible, Faded or Obscured, Missing or Damaged)
[ ] Load Distribution (Consistent and Even, Uneven Distribution, Overloaded Racks (Possible), Under-Utilized Space)
[ ] Notes on Rack Stability (if applicable)
[ ] Location of any rack damage or issues identified.

--- EQUIPMENT & MACHINERY ---
[ ] Forklift Fuel/Battery Level (Percentage)
[ ] Forklift Tire Condition (Good, Fair, Poor - Requires Repair, Flat)
[ ] Conveyor Belt Condition (Operating Normally, Minor Debris, Slippage, Malfunction - Not Operational)
[ ] Notes on Equipment Malfunctions/Issues
[ ] Pallet Jack Condition (Good, Fair, Poor - Requires Repair)
[ ] Hour Meter Reading (e.g., Forklift)

--- CLEANLINESS & HOUSEKEEPING ---
[ ] Are aisles clear of obstructions? (Yes, completely clear, Mostly clear, minor obstructions, Significant obstructions present)
[ ] Is debris (packaging, pallets, etc.) present on the floor? (No debris, Minor debris, Moderate debris, Significant debris)
[ ] Estimate of debris volume (cubic feet):
[ ] Note any spills or leaks (if any):
[ ] Are restroom facilities clean and stocked? (Yes, No)
[ ] Describe any unusual odors detected:

--- SECURITY & ACCESS CONTROL ---
[ ] Are all exterior doors and loading bay doors secured? (Yes, No, N/A)
[ ] Are perimeter fences/gates in good repair? (Yes, No, N/A)
[ ] Are security cameras operational and recording? (Yes, No, N/A)
[ ] Are access control systems (key cards, codes) functioning correctly? (Yes, No, N/A)
[ ] Any suspicious activity observed? If so, describe.
[ ] Number of unauthorized persons observed.

--- ENVIRONMENTAL CONTROL (IF APPLICABLE) ---
[ ] Temperature (degrees Fahrenheit)
[ ] Relative Humidity (%)
[ ] Cooling/Heating System Power Consumption (kWh)
[ ] HVAC Unit Status (Operating Normally, Warning Light Active, Malfunctioning, Off)
[ ] Notes on Environmental Conditions/Equipment Performance
[ ] Dehumidifier Status (if applicable) (Operating Normally, Warning Light Active, Malfunctioning, Off)
[ ] Last Maintenance Date (HVAC/Environmental)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/logistics/daily-warehouse-walkthrough-inspection
(Click "Install Template" to launch your digital inspection tool immediately)