DRONE FLIGHT OPERATIONS CHECKLIST - FARM MANAGEMENT

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-FLIGHT CHECKS ---
[ ] Drone Battery Level (%)
[ ] Propeller Condition (1-5 Scale, 1=Excellent, 5=Damaged)
[ ] GPS Status (Connected, Disconnected, Weak Signal)
[ ] Compass Calibration Required? (Yes, No)
[ ] Time of Pre-Flight Check
[ ] Any unusual noises during motor start?
[ ] Camera Lens Condition (Clean, Smudged, Dirty, Scratched)

--- WEATHER ASSESSMENT ---
[ ] Wind Speed (mph)
[ ] Temperature (Â°F)
[ ] Visibility (miles)
[ ] Cloud Cover (Clear, Few Clouds, Scattered Clouds, Broken Clouds, Overcast)
[ ] Precipitation (None, Light Rain, Moderate Rain, Heavy Rain, Snow, Hail)
[ ] Date of Assessment
[ ] Time of Assessment
[ ] Additional Weather Notes

--- FLIGHT PLANNING & AREA SURVEY ---
[ ] Flight Area Coordinates (GPS)
[ ] Flight Altitude (Feet/Meters)
[ ] Overlap Percentage (Front/Side)
[ ] Flight Purpose (Crop Health Assessment, Field Mapping, Livestock Monitoring, Irrigation Assessment)
[ ] Potential Hazards Identified (e.g., power lines, buildings)
[ ] Planned Flight Date
[ ] Planned Flight Start Time
[ ] Ground Personnel Present (Observer, Spotter, None)

--- REGULATORY COMPLIANCE & PERMISSIONS ---
[ ] FAA Part 107 Certificate Status (Active, Inactive, Pending)
[ ] Certificate Expiration Date
[ ] Airspace Authorization (LAANC) (Approved, Pending, Not Required)
[ ] Flight Altitude (ft)
[ ] Airspace Restrictions & Notices
[ ] Local Regulations Compliance (Compliant, Review Required)
[ ] FAA Authorization Documents (if applicable)

--- DRONE & PAYLOAD INSPECTION ---
[ ] Battery Voltage (V)
[ ] Propeller Condition (1-10)
[ ] Camera Lens Condition (Clean, Slightly Dirty, Dirty, Damaged)
[ ] GPS Signal Strength (Excellent, Good, Fair, Poor)
[ ] Checklist for Obstructions (Propellers, Landing Gear, Sensors, Camera)
[ ] Photo of Drone Condition
[ ] Notes on Drone Condition

--- BATTERY & POWER MANAGEMENT ---
[ ] Battery 1 Voltage (V)
[ ] Battery 2 Voltage (V)
[ ] Battery 1 Capacity (%)
[ ] Battery 2 Capacity (%)
[ ] Battery 1 Condition (Excellent, Good, Fair, Poor)
[ ] Battery 2 Condition (Excellent, Good, Fair, Poor)
[ ] Last Battery Charge Date
[ ] Estimated Flight Time Remaining (mins)

--- GEOFENCE & SAFETY SETTINGS ---
[ ] Maximum Flight Altitude (Feet)
[ ] Return-to-Home Altitude (Feet) (20, 30, 40, 50, Custom)
[ ] Active Safety Features (Obstacle Avoidance, Return-to-Home, Low Battery Warning, Smart Landing)
[ ] Geofence Radius (Feet) (50, 100, 200, 500, Custom)
[ ] Custom Geofence Coordinates (Latitude/Longitude)

--- FLIGHT EXECUTION ---
[ ] Flight Start Time
[ ] Altitude (feet/meters)
[ ] Flight Speed (mph/kmh)
[ ] Flight Mode (Manual, Autonomous, Follow Me)
[ ] Real-time observations during flight (e.g., unusual behavior)
[ ] Battery Percentage Remaining (Estimated)
[ ] Current Drone Location (GPS Coordinates)

--- POST-FLIGHT PROCEDURES ---
[ ] Flight End Time
[ ] Total Flight Time (minutes)
[ ] Flight Log File (Optional)
[ ] Overall Flight Performance (Excellent, Good, Fair, Poor)
[ ] Notes/Observations (e.g., unusual behavior, issues)
[ ] Date of Next Maintenance/Inspection

--- DATA MANAGEMENT & ANALYSIS ---
[ ] Data Analysis Completion Date
[ ] Estimated Crop Yield (based on drone data)
[ ] Summary of Key Insights from Data Analysis
[ ] Data Analysis Priority (for follow-up actions) (High, Medium, Low)
[ ] Exported Data Files (e.g., NDVI maps, point clouds)
[ ] Confidence Level of Data Analysis (0-100)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/farm-management/drone-flight-operations-checklist-farm-management
(Click "Install Template" to launch your digital inspection tool immediately)