ELECTRICAL SAFETY INSPECTION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL INFORMATION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Area/Department Inspected
[ ] Inspector's Name
[ ] Inspector's Title/Role
[ ] Supervising Personnel (if applicable)
[ ] Equipment/Area ID (if applicable)
[ ] Weather Conditions (Optional) (Clear, Rain, Snow, Fog, Other)

--- VISUAL INSPECTION OF EQUIPMENT & WIRING ---
[ ] Inspect for damaged or frayed insulation on cables and wires. (Yes, No, N/A)
[ ] Check for cracked or broken equipment housings and enclosures. (Yes, No, N/A)
[ ] Are there signs of overheating (discoloration, melting)? (Yes, No, N/A)
[ ] Note any cracks, or breaks (count):
[ ] Describe any observed defects or damage:
[ ] Attach photos of any observed damage:
[ ] Condition of wiring supports and conduits: (Good, Fair, Poor)

--- GROUNDING AND BONDING ---
[ ] Is the grounding conductor properly sized according to code? (Yes, No, Not Applicable)
[ ] Are all metal enclosures and equipment properly bonded? (Yes, No, Not Applicable)
[ ] Measured grounding resistance (ohms):
[ ] Is the grounding electrode system adequate? (Yes, No, Not Applicable)
[ ] Notes/Observations regarding grounding and bonding:
[ ] Attach photos of grounding connections (if applicable):

--- OVERCURRENT PROTECTION (CIRCUIT BREAKERS & FUSES) ---
[ ] Circuit Breaker Ampacity (Rated Value)
[ ] Fuse Rating (Amps)
[ ] Circuit Breaker Condition (Good, Damaged, Corroded, Loose, Missing, Other (Specify))
[ ] Fuse Condition (Good, Open, Damaged, Corroded, Missing, Other (Specify))
[ ] Breaker Trip Curve Conformance (Optional â€“ if tested)
[ ] Comments/Observations regarding Overcurrent Protection
[ ] Breaker Labeling Clear and Accurate? (Yes, No, N/A)
[ ] Fuse Marking Present and Legible? (Yes, No, N/A)

--- LOCKOUT/TAGOUT (LOTO) PROCEDURES ---
[ ] Is a written LOTO program available and current? (Yes, No, N/A)
[ ] Are employees trained on the LOTO procedures? (Yes, No, N/A)
[ ] Date of last LOTO training for employees.
[ ] Describe any observed deficiencies in LOTO implementation.
[ ] Which of the following LOTO elements are present and functional? (Lockout Devices, Tagout Devices, Procedures for Group Lockout, Energy Isolation Checks, Stored Energy Documentation)
[ ] Number of documented LOTO incidents in the last year.
[ ] Are energy isolation steps verified before starting work? (Yes, No, N/A)
[ ] Upload a copy of the current LOTO procedure document (if applicable).

--- ELECTRICAL SAFETY DEVICES ---
[ ] Number of GFCI outlets inspected
[ ] GFCI outlet status (per inspection) (Pass, Fail - Needs Repair, Not Present, Not Applicable)
[ ] Number of AFCI breakers inspected (if applicable)
[ ] AFCI breaker status (per inspection - if applicable) (Pass, Fail - Needs Repair, Not Present, Not Applicable)
[ ] Arc Flash Labeling Present on Equipment? (Yes, No, Not Applicable)
[ ] Comments on Arc Flash Labeling or other safety devices
[ ] Emergency Disconnect Switches - Condition (Good, Fair, Poor - Requires Attention)

--- WORK AREA SAFETY ---
[ ] Are walkways and aisles clear of obstructions? (Yes, No, N/A)
[ ] Is adequate lighting provided in work areas? (Yes, No, N/A)
[ ] Distance from electrical equipment to nearest combustible material (inches)
[ ] Check all that apply: What hazards are present in the work area? (Exposed wiring, Damaged equipment, Wet conditions, Overcrowding, None Observed)
[ ] Describe any observed electrical hazards in the work area.
[ ] Are electrical panels accessible and properly labeled? (Yes, No, N/A)

--- EMERGENCY PROCEDURES & SIGNAGE ---
[ ] Are Emergency Contact Numbers Posted? (Yes, No, N/A)
[ ] Are Evacuation Routes Clearly Marked? (Yes, No, N/A)
[ ] Are Emergency Shutdown Procedures Documented? (Yes, No, N/A)
[ ] Describe any issues or observations related to emergency signage.
[ ] Are emergency lighting fixtures functional? (Yes, No, N/A)
[ ] Date of last Emergency Drill
[ ] Name of person responsible for Emergency Procedures

--- EMPLOYEE TRAINING & COMPETENCY ---
[ ] Last Electrical Safety Training Date
[ ] Number of Employees Trained on Electrical Safety
[ ] Training Program Type (Classroom, Online, Hands-on, Combination)
[ ] Topics Covered in Training (Select all that apply) (Lockout/Tagout Procedures, Hazard Identification, Safe Work Practices, Personal Protective Equipment (PPE), Emergency Procedures, NFPA 70E Compliance)
[ ] Brief Summary of Training Content
[ ] Training Records/Certificates (Optional)
[ ] Competency Assessment Method (Written Exam, Practical Assessment, Observation, Combination)

--- RECORD KEEPING ---
[ ] Last Electrical Safety Inspection Date
[ ] Inspection Frequency (e.g., months between inspections)
[ ] Upload Previous Inspection Report
[ ] Summary of Corrective Actions Required (from previous inspection)
[ ] Status of Corrective Actions from Previous Inspection (e.g., Completed, In Progress, Pending)
[ ] Maintenance Records Available (e.g., Yes, No, Partial) (Yes, No, Partial)
[ ] Date of Last Equipment Maintenance Record Reviewed

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/manufacturing/electrical-safety-inspection-checklist
(Click "Install Template" to launch your digital inspection tool immediately)