ELEVATOR AND ESCALATOR SAFETY MAINTENANCE CHECKLIST 2026
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--- CABIN AND CAR INTERIOR INSPECTION ---
[ ] Car Leveling Accuracy (Within Tolerance, Out of Tolerance, Critical Issue)
[ ] Interior Component Condition (Lighting Functioning, Emergency Phone/Intercom Working, Floor Indicator Display Working, Emergency Stop Button Functional, Handrails Secure)
[ ] Observation Notes
[ ] Photo Evidence
[ ] Inspector Verification

--- DOOR AND GATE MECHANISM INSPECTION ---
[ ] Door Sensor Functionality (Operational, Faulty, Requires Repair)
[ ] Track and Rail Condition Notes
[ ] Door Closing Speed (seconds)
[ ] Components Inspected (Door Interlocks, Tracks/Guides, Sensors/Photo-eyes, Door Operators, Manual Release)
[ ] Photo Evidence of Mechanism
[ ] Inspector Verification

--- DRIVE SYSTEM AND MOTOR MAINTENANCE ---
[ ] Motor Lubrication Status (Adequate, Low/Needs Refill, Critical/Leaking)
[ ] Drive Belt Tension (PSI/Newton)
[ ] Brake System Condition (Operational, Worn, Needs Immediate Repair)
[ ] Observations of Gearbox Noise or Vibration
[ ] Upload Motor Service Report/Photos
[ ] Last Component Replacement Date
[ ] Technician Verification

--- ESCALATOR STEP AND HANDRAIL INSPECTION ---
[ ] Step Tread Condition (Good, Worn, Damaged/Broken)
[ ] Handrail Tension and Alignment (Optimal, Loose, Requires Adjustment)
[ ] Comb Plate Integrity (Intact, Missing Teeth, Deformed)
[ ] Handrail Speed (m/s)
[ ] Debris Detected (Dust/Dirt, Metal Shavings, Foreign Objects)
[ ] Deficiency Details
[ ] Photo Evidence of Wear
[ ] Inspection Date

--- SAFETY SENSORS AND EMERGENCY SYSTEMS ---
[ ] Emergency Components Inspected (Emergency Stop Buttons, Fire Service Integration, Overload Sensors, Alarm/Intercom System, Pit Safety Switches)
[ ] Emergency Lighting Status (Operational, Requires Battery Replacement, Non-Functional)
[ ] Sensor Response Time (Seconds)
[ ] Defects or Malfunctions Noted
[ ] Inspector Verification

--- HOISTWAY AND PIT SAFETY CHECK ---
[ ] Inspection Date
[ ] Pit Cleanliness Status (Clean, Debris Present, Requires Immediate Cleaning)
[ ] Guide Rail Lubrication Condition (Adequate, Dry/Low, Excessive/Overflowing)
[ ] Sump Pump Functionality (Operational, Non-Operational, N/A - No Sump Present)
[ ] Components Inspected (Limit Switches, Traveling Cables, Buffer Condition, Guide Rail Brackets)
[ ] Deficiencies or Repair Notes
[ ] Inspector Signature

--- ELECTRICAL AND CONTROL CABINET AUDIT ---
[ ] Inspection Date
[ ] Control Panel Condition (Excellent, Good, Fair, Poor/Requires Repair)
[ ] Components Inspected (Circuit Breakers, Relays and Contactors, Frequency Drives (VFD), Wiring and Terminals, Emergency Stop Circuits)
[ ] Voltage Reading (Main Line)
[ ] Defects or Anomalies Found
[ ] Photo of Control Cabinet Interior
[ ] Technician Verification

--- STRUCTURAL AND LOAD-BEARING COMPONENTS ---
[ ] Guide Rail Condition (Excellent, Good, Needs Repair, Critical Failure)
[ ] Suspension Rope Diameter (mm)
[ ] Observations of Structural Wear or Corrosion
[ ] Components Inspected (Counterweights, Guide Rails, Suspension Ropes, Brackets and Supports)
[ ] Photo Evidence of Load-Bearing Components
[ ] Inspector Verification

--- LUBRICATION AND FLUID MANAGEMENT ---
[ ] Last Lubrication Date
[ ] Gearbox Oil Level Status (Optimal, Low, Critically Low, Needs Refill)
[ ] Guide Rail Lubricant Volume Applied (Liters)
[ ] Components Inspected (Main Drive Gear, Guide Rails, Hydraulic Cylinders, Escalator Chain, Bearing Assemblies)
[ ] Lubrication Notes and Leak Observations
[ ] Photos of Oil/Fluid Condition

--- COMPLIANCE AND DOCUMENTATION LOG ---
[ ] Inspection Date
[ ] Lead Technician Signature
[ ] Compliance Status (Compliant, Non-Compliant, Requires Immediate Action)
[ ] Regulatory Certificate Upload
[ ] Discrepancy Notes and Remediation Plan
[ ] Next Inspection Due Date (Year)
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