ENERGY CONSUMPTION ANALYTICS PROCESS

Created by ChecklistGuro (https://checklistguro.com)

[ ] Fetch Meter Readings: Retrieve all raw energy consumption entries from the Smart Meter Data Model for the specified period.
[ ] Retrieve Utility Tariffs: Get the current pricing and tax rates from the Energy Tariffs Data Model.
[ ] Calculate Total Consumption: Sum the kWh values from the retrieved meter readings to find the total energy used.
[ ] Calculate Total Cost: Multiply the total kWh by the retrieved tariff rate to determine the monetary cost.
[ ] Calculate Peak Usage: Identify the maximum (MAX) energy consumption value recorded in a single interval from the dataset.
[ ] Calculate Average Daily Load: Calculate the average (AVG) daily energy usage to establish a baseline.
[ ] Create Analytics Summary: Generate a new entry in the 'Energy Analytics Report' data model containing the calculated totals, peaks, and costs.
[ ] Identify Anomalies: Compare current usage against historical averages to detect a percentage increase above a specific threshold.
[ ] Assign Data Analyst Review: Create a task for the Energy Analyst to verify the accuracy of the generated analytics summary.
[ ] Maintenance Alert Task: If an anomaly is detected, create a task for the Facilities Manager to inspect the energy hardware.
[ ] Generate Monthly Consumption Report: Compile the aggregated data and summary entries into a formal PDF/Dashboard report.
[ ] Send Summary to Stakeholders: Send an automated email to the Operations Manager with the key findings from the analytics summary.
[ ] Update Baseline Models: Update the 'Historical Baseline' data model with the newly calculated average usage for future comparisons.
[ ] Send Critical Alert SMS: Send an urgent SMS notification to the site supervisor if energy consumption exceeds a critical safety threshold.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/energy/energy-consumption-analytics-process
(Click "Install Template" to launch your digital inspection tool immediately)