ESCALATOR/MOVING WALKWAY MAINTENANCE

Created by ChecklistGuro (https://checklistguro.com)

--- DAILY VISUAL INSPECTION ---
[ ] Overall Condition (Excellent, Good, Fair, Poor)
[ ] Handrail Alignment (Aligned, Slightly Misaligned, Misaligned â€“ Requires Attention)
[ ] Noise Level (1-10, 1=Silent, 10=Very Loud)
[ ] Any Unusual Odors Detected?
[ ] Skirt Condition (Intact, Minor Damage, Significant Damage)
[ ] Step/Tread Condition (Good, Minor Wear, Significant Wear, Damage Present)

--- WEEKLY FUNCTIONAL CHECKS ---
[ ] Step Chain/Belt Speed (ft/min or m/min)
[ ] Step Chain/Belt Tension (lbs or N)
[ ] Step Chain/Belt Alignment (Aligned, Slightly Misaligned, Significantly Misaligned)
[ ] Noise Level (Normal, Slightly Elevated, Excessive)
[ ] Comments/Observations (e.g., unusual noises, vibrations)
[ ] Emergency Stop Buttons Functionality (Functioning Correctly, Requires Attention)
[ ] Motor Current Draw (Amps)

--- MONTHLY PREVENTATIVE MAINTENANCE ---
[ ] Step Chain/Belt Speed (ft/min)
[ ] Motor Amperage (Current Draw)
[ ] Gearbox Oil Level (inches)
[ ] Gearbox Oil Condition (Excellent, Good, Fair, Poor)
[ ] Lubrication Points Inspected/Lubricated (Select all that apply) (Step Chain/Belt, Guide Rails, Bearings, Motor Shaft, Other (Specify in LONG_TEXT))
[ ] If 'Other' selected for lubrication, please specify:
[ ] Comb Condition (Clean, Slightly Dirty, Dirty, Very Dirty)
[ ] Last Filter Replacement Date
[ ] Any unusual noises observed?

--- ANNUAL COMPREHENSIVE MAINTENANCE ---
[ ] Detailed Description of Annual Inspection Findings
[ ] Photographs of Key Components (e.g., Drive System, Step Chains)
[ ] Drive Motor Current Draw (Amps)
[ ] Step Chain Tension (Measured in Inches)
[ ] Gearbox Oil Level (Measured in Inches/Milliliters)
[ ] Gearbox Oil Condition (Visual Inspection) (Excellent, Good, Fair, Poor)
[ ] Date of Next Scheduled Oil Change (Gearbox)
[ ] Areas of Concern Identified (Select all that apply) (Excessive Noise, Vibration, Unusual Odor, Step Misalignment, Electrical Issues, None)
[ ] Recommendations for Corrective Actions
[ ] Technician Signature

--- SAFETY & EMERGENCY SYSTEMS ---
[ ] Last Emergency Stop Test Date
[ ] Emergency Stop Response Time (seconds)
[ ] Emergency Stop Button Condition (Functional/Needs Repair/Out of Service) (Functional, Needs Repair, Out of Service)
[ ] Safety Features Verified (Check all that apply) (Skirting Boards Secure, Comb Plates Clean, Handrails Functional, Emergency Lighting Operational, Fire Detection System Integration, Audible Warnings Functioning)
[ ] Notes on Emergency Response Protocol Review
[ ] Emergency Lighting Battery Status (Good, Fair, Poor - Requires Replacement)
[ ] Photographic Evidence of Safety System Condition

--- DOCUMENTATION & RECORD KEEPING ---
[ ] Date of Last Inspection/Maintenance
[ ] Start Time of Inspection/Maintenance
[ ] Meter Reading (Total Steps/Distance)
[ ] Observations & Notes (Describe any issues found)
[ ] Condition of Escalator/Moving Walkway (Post-Maintenance) (Excellent, Good, Fair, Poor)
[ ] Upload Photos/Videos (Evidence of condition or repairs)
[ ] Technician Name
[ ] Contractor (If applicable)
[ ] Recommendations for Future Maintenance

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/facility-management/escalator-moving-walkway-maintenance
(Click "Install Template" to launch your digital inspection tool immediately)