FARM EQUIPMENT INSPECTION AND MAINTENANCE CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-OPERATION INSPECTION ---
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Equipment Hour Meter Reading
[ ] Operator Name (Select Operator, Operator 1, Operator 2, Operator 3)
[ ] Equipment Condition (Pre-Operation) (Select Condition, Excellent, Good, Fair, Poor)
[ ] Notes/Observations (Pre-Operation)
[ ] Location of Equipment
[ ] Operator Signature

--- ENGINE & POWERPLANT ---
[ ] Engine Hours
[ ] Oil Level (in inches)
[ ] Oil Condition (Clean, Slightly Dirty, Dirty, Contaminated)
[ ] Coolant Level (Full, Low, Empty)
[ ] Coolant Temperature (during operation, Â°F)
[ ] Notes on Engine Performance
[ ] Fuel Filter Condition (Good, Fair, Poor)
[ ] Photo of Engine Bay

--- HYDRAULIC SYSTEM ---
[ ] Hydraulic Fluid Level (inches)
[ ] Hydraulic Fluid Condition (Good, Cloudy, Contaminated, Milky)
[ ] Hose Condition (Excellent, Good, Fair, Poor, Leaking)
[ ] Cylinder Extension Speed (seconds)
[ ] Notes on Hydraulic System Performance
[ ] Pump Noise Level (Normal, Slightly Elevated, Loud, Unusual)
[ ] Photo of Hydraulic Lines (if any leaks)

--- TIRES & TRACKS ---
[ ] Tire Pressure (PSI)
[ ] Track Depth (inches)
[ ] Tire Condition (Excellent, Good, Fair, Poor)
[ ] Track Condition (Excellent, Good, Fair, Poor)
[ ] Notes on Tire/Track Damage or Wear
[ ] Tire Issues? (Cuts, Bulges, Cracks, Wear Bars Visible)
[ ] Attach Tire/Track Photos

--- IMPLEMENTS & ATTACHMENTS ---
[ ] Mower Deck Condition (Excellent, Good, Fair, Poor)
[ ] Tire Pressure (Rear - PSI)
[ ] Hitch Condition (No Issues, Minor Rust, Significant Damage, Needs Repair)
[ ] Notes on Attachment Performance
[ ] Which implements are attached? (Moldboard Plow, Disc Harrow, Cultivator, Grain Drill, Sprayer)
[ ] Sprayer Tank Volume (Gallons)
[ ] Blade Sharpness (Sharp, Dull, Needs Sharpening)

--- SAFETY EQUIPMENT ---
[ ] ROPS (Roll-Over Protective Structure) Condition (Intact & Secure, Damaged, Missing)
[ ] Seatbelt Condition (Present & Functional, Damaged, Missing)
[ ] Lights (Headlights, Taillights, Turn Signals) Functionality (All Functioning, Some Not Functioning, None Functioning)
[ ] Fire Extinguisher Inspection Date
[ ] Backup Alarm Operational? (Yes, No, N/A)
[ ] Photo Evidence of Safety Equipment

--- LUBRICATION & FLUIDS ---
[ ] Engine Oil Level (in quarts)
[ ] Hydraulic Oil Level (in quarts)
[ ] Transmission Fluid Level (in quarts)
[ ] Engine Oil Condition (Excellent, Good, Fair, Poor)
[ ] Hydraulic Oil Condition (Excellent, Good, Fair, Poor)
[ ] Date of Last Oil Change
[ ] Coolant Level (in quarts)
[ ] Notes on Fluid Levels or Condition

--- ELECTRICAL SYSTEM ---
[ ] Battery Voltage (DC)
[ ] Wiring Condition (Excellent, Good, Fair, Poor)
[ ] Lights Functionality (Headlights, Taillights, Turn Signals) (All Functioning, Some Malfunctioning, None Functioning)
[ ] Notes on Electrical Components or Issues
[ ] Generator Output Voltage (if applicable)
[ ] Wiring Insulation Condition (Intact, Cracked, Exposed, Damaged)

--- GENERAL CONDITION ---
[ ] Describe any visible signs of damage or corrosion
[ ] Estimated Operating Hours (Current)
[ ] Check all that apply: Evidence of leaks? (Hydraulic Fluid, Engine Oil, Coolant, None Observed)
[ ] Overall Condition Rating (1-5, 1=Poor, 5=Excellent)
[ ] Notes on Paint/Decals Condition
[ ] Date of Last Major Repair

--- POST-OPERATION MAINTENANCE ---
[ ] Date of Last Maintenance
[ ] Operating Hours Since Last Maintenance
[ ] Notes on Operation or Maintenance Performed
[ ] Fluid Levels Checked? (Yes, No)
[ ] Filters Inspected? (Yes, No)
[ ] Tire Pressure (PSI)
[ ] Lubrication Points Greased? (Grease Fittings, Chain Lubrication, Other)
[ ] Time of Post-Operation Inspection

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/inspection-management/farm-equipment-inspection-and-maintenance-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)