FIRE SPRINKLER SYSTEM INSTALLATION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-INSTALLATION PLANNING & PERMITS ---
[ ] Project Start Date
[ ] Project Description & Scope of Work
[ ] Authority Having Jurisdiction (AHJ) (Local Fire Marshal, City Fire Department, State Fire Marshal, Other (Specify in LONG_TEXT))
[ ] Approved Sprinkler System Shop Drawings
[ ] Permit Number
[ ] Permit Status (Applied For, Approved, Pending Review, Rejected)
[ ] Notes on Permit Approval/Rejection

--- SITE PREPARATION & LAYOUT ---
[ ] Existing Utility Location Verification
[ ] Sprinkler System Layout Marked on Site
[ ] Elevation Difference for Pipe Slope (if applicable)
[ ] Ground Condition Assessment (e.g., stable, unstable, rocky) (Stable, Unstable, Rocky, Sandy)
[ ] Date of Site Survey/Layout Verification
[ ] Notes on Site Preparation (e.g., obstructions, access limitations)

--- PIPE INSTALLATION & SUPPORT ---
[ ] Pipe Diameter (inches)
[ ] Pipe Material Thickness (schedule)
[ ] Pipe Material Type (Steel (Black), Steel (Galvanized), CPVC, PEX, Other (Specify in LONG_TEXT))
[ ] If 'Other' Pipe Material Selected, Please Specify:
[ ] Number of Pipe Hangers Installed
[ ] Hanger Spacing Verified? (Yes, No)
[ ] If Hanger Spacing Not Verified, Explain:
[ ] Pipe Alignment Verified? (Yes, No)
[ ] Pipe Installation Photos

--- SPRINKLER HEAD INSTALLATION ---
[ ] Sprinkler Head ID (Sequential)
[ ] Sprinkler Head Type (Standard Spray, Pendent, Sidewall, Concealed, Upright)
[ ] Sprinkler Head Orientation (Upward, Downward, Horizontal)
[ ] Sprinkler Head Temperature Rating (degrees F)
[ ] Sprinkler Head Location (Grid Coordinates or Description)
[ ] Manufacturer & Model Number
[ ] Distance from Wall (inches)
[ ] Sprinkler Head Condition (Post Install) (Satisfactory, Minor Defect - Notified, Major Defect - Rework Required)
[ ] Notes/Comments regarding installation

--- RISER INSTALLATION ---
[ ] Riser Pipe Diameter (inches)
[ ] Riser Material Type (Steel, CPVC, Galvanized Steel, Other)
[ ] Number of Risers Installed
[ ] Riser Location (coordinates/description)
[ ] Riser Installation Completion Date
[ ] Details of Riser Support System (type, spacing)
[ ] Riser Insulation Type (if applicable) (None, Fiberglass, Foam, Other)
[ ] Hydrostatic Test Pressure (PSI)

--- CONTROL VALVE & ALARM PANEL INSTALLATION ---
[ ] Control Valve Size (inches)
[ ] Control Valve Type (OS&Y, Butterfly, Gate, Ball)
[ ] Alarm Panel Model Number
[ ] Alarm Panel Wiring Diagram Verification Notes
[ ] Alarm Panel Programming Completion Date
[ ] Supervisory Switch Settings (PSI)
[ ] Tamper Switch Functionality Test Result (Pass, Fail, NA)
[ ] Control Valve Labeling Verification (Yes/No)

--- FIRE DEPARTMENT CONNECTION (FDC) ---
[ ] FDC Connection Size (inches)
[ ] FDC Valve Type (Butterfly Valve, Gate Valve, Other (Specify))
[ ] If 'Other' valve type selected, specify:
[ ] FDC Signage Present & Visible? (Yes, No)
[ ] If 'No' signage present, provide explanation:
[ ] Date of FDC Inspection
[ ] Time of FDC Inspection
[ ] FDC Pressure (PSI)
[ ] Upload Photo of FDC Installation

--- SYSTEM TESTING & FLUSHING ---
[ ] Hydrostatic Test Pressure (PSI)
[ ] Hydrostatic Test Duration (Minutes)
[ ] Flow Test Pressure (PSI)
[ ] Flow Rate (GPM)
[ ] Flush Water Clarity (Clear, Slightly Cloudy, Cloudy)
[ ] Notes on Flush Water Clarity (if not Clear)
[ ] Hydrostatic Test Date
[ ] Hydrostatic Test Time
[ ] Hydrostatic Test Record/Graph

--- DOCUMENTATION & AS-BUILT DRAWINGS ---
[ ] Original System Design Drawings
[ ] Permit Documentation (Approved Plans, Inspection Reports)
[ ] Description of Deviations from Original Design (if any)
[ ] As-Built Drawings (Signed and Dated)
[ ] Date of As-Built Drawing Completion
[ ] Hydrostatic Test Pressure (in PSI)
[ ] Hydrostatic Test Duration (in minutes)
[ ] Contractor Representative Signature
[ ] Owner/Client Representative Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/fire-sprinkler-system-installation-checklist
(Click "Install Template" to launch your digital inspection tool immediately)