FLEET FUELING STATION COMPLIANCE AND SAFETY INSPECTION CHECKLIST 2026
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--- FUEL STORAGE TANK INTEGRITY & MONITORING ---
[ ] Inspection Date
[ ] Tank ID/Storage Unit Number
[ ] Visual Leak Inspection Status (No Leaks Detected, Minor Seepage Noted, Major Leak Detected)
[ ] Current Fuel Level (Gallons/Liters)
[ ] Secondary Containment Condition (Intact & Dry, Debris/Sediment Present, Evidence of Fluid Accumulation)
[ ] Observations and Maintenance Notes
[ ] Upload Photo of Tank Gauges/Integrity
[ ] Inspector Signature

--- DISPENSING EQUIPMENT & HOSE INSPECTION ---
[ ] Inspection Date
[ ] Nozzle Condition (Good, Worn/Damaged, Leaking)
[ ] Hose Integrity Check (No cracks or abrasions detected, Visible cracks or surface damage, Significant leaks or swelling)
[ ] Hose Age (Months)
[ ] Detected Issues (Leaking Nozzle, Cracked Hose, Broken Breakaway, Faulty Meter/Display)
[ ] Detailed Repair Notes
[ ] Photo of Equipment Damage
[ ] Inspector Signature

--- EMERGENCY SHUTDOWN & FIRE SUPPRESSION SYSTEMS ---
[ ] Emergency Shutdown Button Status (Operational/Functional, Non-Functional/Requires Repair, Not Applicable)
[ ] Fire Extinguisher Pressure Check (In Green Zone (Charged), In Red Zone (Depressurized), Missing/Not Found)
[ ] Last Fire Suppression System Service Date
[ ] Deficiencies or Repairs Required
[ ] Photo Evidence of Equipment Condition
[ ] Inspector Verification

--- CONTAINMENT & SPILL PREVENTION CONTROLS ---
[ ] Secondary Containment Integrity Status (Intact - No visible leaks or debris, Maintenance Required - Minor cracks or buildup, Critical Issue - Active leak or breach detected)
[ ] Spill Kit Inventory Checklist (Absorbent Pads, Absorbent Socks/Booms, Disposal Bags & Ties, Neutralizing Agents, Drain Covers)
[ ] Oil-Water Separator Maintenance Interval (Days)
[ ] Photo Evidence of Containment Area
[ ] Spill Prevention Corrective Actions
[ ] Inspector Verification

--- ELECTRICAL & GROUNDING SAFETY ---
[ ] Grounding Wire Integrity Status (Secure and Undamaged, Corroded or Loose, Missing or Severed)
[ ] Explosion-Proof Lighting Condition (Operational/Intact, Damaged/Cracked Lens, Non-functional)
[ ] Voltage Reading (Main Panel)
[ ] Observed Electrical Anomalies
[ ] Corrective Action Required
[ ] Inspector Verification

--- SIGNAGE, LABELING & REGULATORY COMPLIANCE ---
[ ] Hazard Signage Condition (Clear and Visible, Faded/Damaged, Missing)
[ ] Emergency Contact Information Visibility (Compliant, Non-Compliant)
[ ] Required Regulatory Labels Present (Flammable Liquid Warnings, No Smoking Prohibitions, Tank Contents Identification, Maximum Capacity Marks)
[ ] Discrepancies or Missing Signage Details
[ ] Photo Evidence of Compliance
[ ] Last Regulatory Permit Review Date
[ ] Inspector Attestation

--- SITE PERIMETER & SECURITY ASSESSMENT ---
[ ] Perimeter Fencing Integrity (Intact and Secure, Damaged/Breached, Needs Maintenance)
[ ] Security Lighting Functionality (All lights operational, Partial outage detected, Significant dark spots identified)
[ ] Security Features Inspected (CCTV Cameras, Motion Sensors, Access Gates, Security Lighting, Perimeter Fencing)
[ ] Security Vulnerability Observations
[ ] Site Perimeter Photos
[ ] Inspector Verification

--- PERSONNEL SAFETY & PPE AVAILABILITY ---
[ ] Available PPE Items Verified (Safety Gloves, Safety Goggles/Face Shields, High-Visibility Vests, Nitrile/Chemical Resistant Gloves, Eye Wash Station Access)
[ ] PPE Condition Status (All items in good condition, Some items require replacement, Critical PPE missing/damaged)
[ ] PPE Deficiency Details
[ ] Safety Officer Verification
[ ] Inspection Date
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