FOOD PROCESSING LINE AND PACKAGING MACHINERY MAINTENANCE CHECKLIST 2026

Created by ChecklistGuro (https://checklistguro.com)


--- PRE-OPERATIONAL INSPECTION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Production Line ID/Area
[ ] Pre-Start Safety Check Components (Emergency Stops Functional, Guards and Shields in Place, No Visible Loose Debris, All Sensors Operational)
[ ] Machine Power Status (Ready for Operation, Maintenance Required, Out of Service)
[ ] Observed Anomalies or Pre-Start Issues
[ ] Inspector Signature

--- SANITATION AND HYGIENE VERIFICATION ---
[ ] Inspection Date
[ ] Sanitation Protocol Status (Fully Sanitized, Partial Cleaning Performed, Re-cleaning Required)
[ ] Surfaces Inspected (Food-Contact Surfaces, Conveyor Belts, Packaging Trays, Nozzles and Injectors, Structural Framework)
[ ] Residual Residue Detected
[ ] Cleaning Discrepancies or Issues Found
[ ] Upload Photo of Cleaned Area
[ ] Sanitation Supervisor Signature

--- CONVEYOR AND BELT SYSTEM MAINTENANCE ---
[ ] Inspection Date
[ ] Belt Tension Status (Optimal, Loose, Too Tight)
[ ] Observed Issues (Belt Misalignment, Surface Wear/Tearing, Debris Accumulation, Roller/Idler Malfunction)
[ ] Measured Belt Tension (Newtons/lbs)
[ ] Maintenance Notes and Observations
[ ] Technician Signature

--- PACKAGING AND SEALING EQUIPMENT CHECK ---
[ ] Sealer Temperature Status (Optimal, Too Low, Too High, Inconsistent)
[ ] Inspected Components (Heat Sealing Bars, Vacuum Pump, Label Applicator, Cutting Blades, Pressure Rollers)
[ ] Seal Integrity Pressure (PSI)
[ ] Seal Quality Observations
[ ] Post-Check Photo Evidence
[ ] Technician Verification

--- LUBRICATION AND FLUID MANAGEMENT ---
[ ] Lubricant Type Used (Food-Grade Synthetic Oil, Food-Grade Grease, Mineral Oil, Other)
[ ] Fluid Level (Liters/Units)
[ ] Tasks Completed (Refilled Reservoir, Greased Bearings, Inspected for Leaks, Drained Old Fluid)
[ ] Observations or Leak Details
[ ] Next Lubrication Due Date
[ ] Technician Authorization

--- ELECTRICAL AND CONTROL SYSTEM INSPECTION ---
[ ] Inspection Date
[ ] Emergency Stop Button Functionality (Operational, Faulty, Needs Repair)
[ ] Control Panel Condition (Clean and Intact, Dust/Debris Present, Corrosion Detected)
[ ] Voltage Reading (Main Supply)
[ ] Sensors Checked (Proximity Sensors, Photoelectric Sensors, Temperature Sensors, Pressure Sensors)
[ ] Electrical Fault Observations
[ ] Photo of Electrical Panel Condition
[ ] Technician Signature

--- MECHANICAL DRIVE AND MOTOR INSPECTION ---
[ ] Inspection Date
[ ] Motor Temperature Status (Normal, Overheating, Critical)
[ ] Measured Motor Temperature (°C)
[ ] Drive Component Inspection Items (Drive Belt Tension, Gearbox Oil Levels, Bearing Lubrication, Chain Tension/Wear)
[ ] Observations and Anomalies
[ ] Technician Signature

--- PNEUMATIC AND HYDRAULIC SYSTEM CHECK ---
[ ] Inspection Date
[ ] Air Pressure Level Status (Normal, Low Pressure, Critical/Low)
[ ] Measured PSI/Bar Reading
[ ] Observed Leak Locations (Hydraulic Hoses, Pneumatic Fittings, Cylinders, Valves, Air Compressor Lines)
[ ] Leakage or Leak Description
[ ] Technician Signature

--- METAL DETECTOR AND X-RAY INSPECTION VERIFICATION ---
[ ] Inspection Date
[ ] Test Piece Type Used (Ferrous (Fe), Non-Ferrous (Non-Fe), Stainless Steel (SS))
[ ] Detection Result (Pass - All test pieces detected, Fail - System failed to detect)
[ ] Sensitivity Setting (mm)
[ ] Discrepancies or Rejection Issues Noted
[ ] Calibration Certificate / Test Report
[ ] Inspector Signature

--- POST-MAINTENANCE DOCUMENTATION ---
[ ] Completion Date
[ ] Technician Name
[ ] Maintenance Summary & Findings
[ ] Parts Replaced (Belts/Conveyors, Bearings, Lubricants, Sensors/Electrical, Seal/Gaskets)
[ ] Photos of Completed Work
[ ] Technician Signature
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