FRAMING MATERIAL INSPECTION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- MATERIAL VERIFICATION ---
[ ] Material Type Specified? (Yes, No)
[ ] Lumber Grade Specified? (Yes, No)
[ ] Steel Gauge Specified (if applicable)? (Yes, No)
[ ] Quantity Received
[ ] Quantity Ordered
[ ] Material Matches Specifications? (Yes, No)
[ ] Discrepancy Notes
[ ] Delivery Ticket/Manifest

--- DELIVERY & STORAGE ---
[ ] Delivery Date
[ ] Delivery Method (Truck, Rail, etc.) (Truck, Rail, Other)
[ ] Condition of Delivery Vehicle (Good, Fair, Poor)
[ ] Notes on Vehicle Condition (if applicable)
[ ] Material Secured During Transit? (Yes, No, N/A)
[ ] Description of Storage Area
[ ] Material Protected from Weather? (Yes, No, Partially)
[ ] Observations Regarding Storage (e.g., level surface, covered, etc.)

--- LUMBER QUALITY ---
[ ] Presence of Wane (reduced width due to loss of wood) (None, Minor, Moderate, Significant, Unacceptable)
[ ] Presence of Knots (None, Small/Tight, Medium, Large/Loose, Unacceptable)
[ ] Straightness Deviation (inches per 16 feet)
[ ] Description of any Visible Defects
[ ] Grade Stamp Verification (Present & Legible, Present & Difficult to Read, Missing, Not Applicable)
[ ] Moisture Content (%)
[ ] Bending/Bow (None, Minor, Moderate, Severe)

--- STEEL FRAMING QUALITY (IF APPLICABLE) ---
[ ] Steel Gauge (Thickness)
[ ] Steel Grade (e.g., G60, G90) (G60, G90, Other (Specify))
[ ] Coating Type (e.g., Galvanized, Zinc-Plated) (Galvanized, Zinc-Plated, Other (Specify))
[ ] Coating Description (if 'Other' is selected)
[ ] Straightness Deviation (Maximum allowed)
[ ] Edge Condition (e.g., Sharp, Rounded) (Sharp, Rounded, Other (Specify))
[ ] Edge Condition Description (if 'Other' is selected)
[ ] Upload Photo of Steel Frame (representative sample)

--- FASTENERS ---
[ ] Nail/Screw Gauge (inches)
[ ] Nail/Screw Length (inches)
[ ] Nail/Screw Type (Common Nail, Box Nail, Drywall Nail, Deck Screw, Construction Screw, Other (Specify))
[ ] Material Coating (Check all that apply) (Galvanized, Stainless Steel, Hot-Dip Galvanized, None)
[ ] Adherence to Specification (Compliant, Non-Compliant, NA)
[ ] Notes/Observations (e.g., rust, damage, inconsistencies)
[ ] Photo Documentation (if non-compliant)

--- MOISTURE CONTENT ---
[ ] Average Moisture Content (%)
[ ] Maximum Allowable Moisture Content (%)
[ ] Minimum Allowable Moisture Content (%)
[ ] Moisture Meter Type (Pin Type, Pinless, Other)
[ ] Notes on Moisture Readings (e.g., areas of high moisture)
[ ] Moisture Content Within Specifications? (Yes, No, N/A)
[ ] Moisture Meter Calibration Certificate (if available)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/framing-material-inspection-checklist
(Click "Install Template" to launch your digital inspection tool immediately)