HVAC SYSTEM PERFORMANCE - PRODUCTION AREAS

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL SYSTEM OVERVIEW & MONITORING ---
[ ] Overall System Runtime (Hours)
[ ] Total Production Area CFM (Cubic Feet per Minute)
[ ] Average Production Area Temperature (Degrees)
[ ] Average Production Area Humidity (%)
[ ] Overall System Status (Nominal, Warning, Critical)
[ ] Any Unusual Observations During Inspection
[ ] Last System Performance Review Date
[ ] System Performance Graph/Report (if available)

--- AIRFLOW & VENTILATION ---
[ ] Measured Airflow (CFM/m³/min) at Supply Diffusers - Area 1
[ ] Measured Airflow (CFM/m³/min) at Return Grilles - Area 1
[ ] Static Pressure at Fan (in WC/Pa)
[ ] Air Distribution Pattern (Observe & Select) (Uniform, Drafty, Uneven, As Expected)
[ ] Supply Air Volume Damper Operation (Fully Open, Partially Open, Closed, Malfunctioning)
[ ] Notes on Airflow Observations (e.g., drafts, stagnant areas)
[ ] Location of observed airflow issues

--- TEMPERATURE & HUMIDITY CONTROL ---
[ ] Production Area 1 - Target Temperature (deg F)
[ ] Production Area 1 - Actual Temperature (deg F)
[ ] Production Area 1 - Target Humidity (%)
[ ] Production Area 1 - Actual Humidity (%)
[ ] Production Area 1 - Temperature Control Mode (Cooling, Heating, Off, Automatic)
[ ] Production Area 1 - Humidity Control Mode (Dehumidifying, Humidifying, Off, Automatic)
[ ] Notes/Observations for Production Area 1 - Temperature/Humidity
[ ] Date of Temperature/Humidity Readings - Production Area 1

--- EQUIPMENT CONDITION & PERFORMANCE ---
[ ] Supply Air Temperature (SAT) - Production Area 1 (°C)
[ ] Return Air Temperature (RAT) - Production Area 1 (°C)
[ ] Supply Air Volume (CFM/m³/min) - Production Area 1
[ ] Chiller/Cooling Tower Efficiency (%)
[ ] Compressor Status (Cooling System) (Operating Normally, Warning, Fault)
[ ] Fan Motor Condition (Main Air Handler) (Normal, Noise/Vibration, Overheating)
[ ] Observations regarding equipment performance (noise, vibration, leaks, etc.)
[ ] Last Maintenance Date - Main Air Handler

--- FILTRATION & AIR QUALITY ---
[ ] MERV Rating of Filters in Use
[ ] Pressure Drop Across Filters (in)
[ ] Filter Replacement Schedule Followed? (Yes, No, N/A)
[ ] Particulate Matter (PM2.5) Reading (µg/m³)
[ ] Any noticeable odors or air quality concerns observed?
[ ] Evidence of Dust Accumulation on Equipment? (Yes, No, Minor, Significant)
[ ] Date of Last Filter Change

--- ENERGY EFFICIENCY & OPTIMIZATION ---
[ ] Average Energy Consumption (kWh)
[ ] Peak Demand (kW)
[ ] Coefficient of Performance (COP) - Cooling Mode
[ ] Coefficient of Performance (COP) - Heating Mode
[ ] Economizer Mode Status (Enabled & Functioning, Enabled & Not Functioning, Disabled, Not Applicable)
[ ] Variable Frequency Drive (VFD) Optimization Status (Optimized, Requires Review, Not Applicable)
[ ] Observations & Recommendations for Energy Savings
[ ] Date of Last Energy Audit

--- SAFETY & MAINTENANCE COMPLIANCE ---
[ ] Last Preventative Maintenance Date
[ ] Maintenance Log Review Frequency (Months)
[ ] Maintenance Performed by (Internal/External) (Internal, External)
[ ] Brief Description of Maintenance Performed
[ ] Safety Inspection Completed? (Yes, No)
[ ] Last Safety Inspection Date
[ ] Safety Inspection Findings & Corrective Actions
[ ] Upload Maintenance Records/Certifications

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/facility-management/hvac-system-performance-production-areas
(Click "Install Template" to launch your digital inspection tool immediately)