INTERIOR PAINTING CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-PAINTING PREPARATION ---
[ ] Describe the Scope of Work
[ ] Room Type (Living Room, Bedroom, Bathroom, Kitchen, Hallway, Other)
[ ] Approximate Square Footage
[ ] Identify Existing Condition (Check all that apply) (New Construction, Previously Painted, Water Damage, Mold/Mildew, Cracks/Holes, Wallpaper Removal Required)
[ ] Note any unusual features or concerns
[ ] Attach Photos of Existing Condition

--- SURFACE PREPARATION ---
[ ] Describe existing surface condition (e.g., wallpaper, existing paint type, damage)
[ ] Identify and address any surface defects: (Cracks, Holes, Loose Paint/Wallpaper, Mold/Mildew, Stains (water, smoke, grease), None)
[ ] If patching, amount of patching compound used (lbs/kg)
[ ] Detail patching/repair procedures followed.
[ ] Surface cleaning method used: (TSP Wash, Mild Detergent Wash, Specialized Cleaner, None (Surface Clean))
[ ] Number of coats of primer applied.
[ ] Type of primer used: (Oil-Based, Latex/Water-Based, Specialty Primer (e.g., stain-blocking))
[ ] Record any issues encountered during surface preparation and corrective actions taken.
[ ] Upload photos of surface condition before and after preparation

--- PAINTING APPLICATION ---
[ ] Number of Paint Coats Applied (per surface)
[ ] Painting Technique Used (e.g., brushing, rolling, spraying) (Brushing, Rolling, Spraying, Other (Specify))
[ ] Notes on Application (e.g., any challenges, specific areas needing extra attention)
[ ] Paint Drying Time (Manufacturer Recommendation) (Less than 2 hours, 2-4 hours, 4-6 hours, 6+ hours)
[ ] Ambient Temperature During Painting (°C or °F)
[ ] Surface Temperature During Painting (°C or °F)
[ ] Details of any problem areas encountered during application and resolution.

--- POST-PAINTING CLEANUP & INSPECTION ---
[ ] Check areas for drips and splatters. (Walls, Floors, Trim, Ceilings, Furniture)
[ ] Number of touch-up areas identified.
[ ] Detailed description of touch-up areas and actions taken.
[ ] Paint finish satisfactory? (Yes, No)
[ ] If 'No', describe the issue with the paint finish.
[ ] Cleanup of painting supplies completed? (Yes, No)
[ ] Cleanup Items Verified (Paint cans, Brushes/Rollers, Drop cloths, Tape, Rags)
[ ] Contractor Signature (Verification of Completion)
[ ] Date of Inspection & Completion

--- SAFETY & ENVIRONMENTAL CONSIDERATIONS ---
[ ] PPE Required (Check all that apply) (Safety Glasses, Gloves, Respirator, Hearing Protection, Coveralls)
[ ] SDS (Safety Data Sheet) Review
[ ] Ventilation Rate (CFM)
[ ] Waste Disposal Method (Recycling, Hazardous Waste Disposal, General Waste)
[ ] Spill Response Plan
[ ] Last Date of Safety Training Review
[ ] Proof of Ventilation System Certification (if applicable)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/interior-painting-checklist
(Click "Install Template" to launch your digital inspection tool immediately)