LNG FACILITY SAFETY & INSPECTION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-OPERATION CHECKS ---
[ ] Planned Startup Date
[ ] Scheduled Startup Time
[ ] Ambient Temperature (Celsius)
[ ] Wind Speed (m/s)
[ ] Weather Conditions (Clear, Cloudy, Rain, Fog, Snow)
[ ] Pre-Startup Checklist Review Notes
[ ] Operator Signature - Pre-Startup Verification

--- TANK & VESSEL INSPECTIONS ---
[ ] Tank Wall Thickness (mm)
[ ] Tank Pressure (kPa)
[ ] Corrosion Observations
[ ] Crack or Weld Defect Notes
[ ] Level Gauge Status (Functional, Malfunctioning, Needs Calibration)
[ ] Tank Inspection Photos
[ ] Last Internal Inspection Date
[ ] Vessel Material Type (Carbon Steel, Stainless Steel, Other)

--- PIPELINE INTEGRITY ---
[ ] Pipeline Operating Pressure (PSI)
[ ] Pipeline Wall Thickness (inches)
[ ] Pipeline Material Type (Carbon Steel, Stainless Steel, Other)
[ ] Last Internal Inspection Date
[ ] Time of Inspection Start
[ ] Corrosion Rate (mm/year)
[ ] Pigging Frequency (Months) (Every 1-3 Months, Every 3-6 Months, Every 6-12 Months, Longer than 12 Months)
[ ] GPS Coordinates of Inspection Location

--- FIRE PROTECTION SYSTEMS ---
[ ] Fire Water Tank Level (Gallons)
[ ] Fire Pump Condition (Operational, Needs Maintenance, Out of Service)
[ ] Last Fire Extinguisher Inspection Date
[ ] Sprinkler System Valve Status (Open, Closed, Partially Open)
[ ] Fire Hose Pressure (PSI)
[ ] Fire Alarm Panel Status (Normal, Fault, Testing)
[ ] Comments/Observations Regarding Fire Protection Systems

--- GAS DETECTION & MONITORING ---
[ ] Methane Concentration (ppm)
[ ] Hydrogen Sulfide Concentration (ppm)
[ ] Ambient Temperature (Â°C)
[ ] Detector Calibration Status (Calibrated, Needs Calibration, Out of Service)
[ ] Last Calibration Date
[ ] Time of Reading
[ ] Detector Location(s) Checked (Tank Farm, Loading Dock, Control Room, Pipeline Access Points)
[ ] Detector Malfunction/Alarm Notes

--- ELECTRICAL SAFETY ---
[ ] Voltage Reading (Phase A)
[ ] Voltage Reading (Phase B)
[ ] Voltage Reading (Phase C)
[ ] Grounding System Condition (Excellent, Good, Fair, Poor)
[ ] Potential Hazards Observed (Exposed Wiring, Damaged Insulation, Loose Connections, Lack of Grounding, Overheating Equipment, None Observed)
[ ] Notes on Electrical Equipment Condition
[ ] Last Electrical Inspection Date
[ ] Inspector Signature

--- SECURITY SYSTEMS ---
[ ] Perimeter Fence Height (meters)
[ ] CCTV System Status (Operational, Degraded, Non-Operational)
[ ] Access Control Points Checked (Main Gate, Service Entrance, Loading Dock, Administration Building)
[ ] Last Intrusion Detection System Test Date
[ ] Time of Security Patrol Start
[ ] Location of Security Control Room

--- PERSONNEL TRAINING & COMPETENCY ---
[ ] Last Hazmat Training Date (Within Last 6 Months, Within Last 12 Months, More than 12 Months, Not Required)
[ ] Last Emergency Response Drill Date
[ ] Number of Hours of LNG Handling Training
[ ] Relevant Certifications (OSHA 10, OSHA 30, First Aid/CPR, Confined Space Entry, HAZWOPER)
[ ] Trainee Signature
[ ] Training Deficiencies Noted (if any)

--- ENVIRONMENTAL COMPLIANCE ---
[ ] Last Emissions Monitoring Date
[ ] Methane Emission Levels (ppm)
[ ] Spill Prevention Plan Status (Up-to-date, Needs Review, Outdated)
[ ] Summary of Recent Environmental Audits
[ ] Environmental Monitoring Reports
[ ] Waste Management Plan Compliance (Compliant, Minor Deviation, Significant Deviation)

--- POST-OPERATION CHECKS ---
[ ] Shutdown Completion Time
[ ] Final Tank Pressure (psia)
[ ] All Systems Verified Offline? (Yes, No)
[ ] Date of Last Shutdown
[ ] Abnormalities/Observations During Shutdown
[ ] Operator Signature (Confirmation of Shutdown)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/energy/lng-facility-safety-inspection-checklist
(Click "Install Template" to launch your digital inspection tool immediately)