LOADING DOCK AND DOCK LEVELER MAINTENANCE INSPECTION CHECKLIST 2026
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--- DOCK LEVELER MECHANICAL INSPECTION ---
[ ] Inspection Date
[ ] Leveler Operational Status (Fully Functional, Functional with Minor Issues, Requires Immediate Repair, Out of Service)
[ ] Mechanical Components Inspected (Hydraulic Cylinders, Hinges and Pivot Points, Spring Tensioners, Structural Support Beams, Lip Mechanism)
[ ] Detailed Mechanical Observations
[ ] Photo Evidence of Mechanical Components
[ ] Inspector Signature

--- DOCK PLATE AND DECK CONDITION ---
[ ] Overall Deck Condition (Excellent, Good, Fair, Poor)
[ ] Identified Defects (Surface Cracks, Dents or Warping, Structural Rust, Loose Bolts/Fasteners, None)
[ ] Defect Details and Repair Notes
[ ] Photo of Deck Condition
[ ] Inspection Date

--- DOCK BUMPERS AND SEALS ---
[ ] Bumper Condition (Good, Worn, Damaged/Needs Replacement)
[ ] Bumper Attachment Security
[ ] Dock Seal Integrity (Intact, Torn/Damaged, Degraded/Compressed)
[ ] Damage Description and Repairs Needed
[ ] Photo of Damaged Bumpers or Seals

--- DOCK LEVELER PIT AND HYDRAULIC SYSTEM ---
[ ] Inspection Date
[ ] Hydraulic Fluid Level Status (Optimal, Low, Critical/Refill Required)
[ ] Visible Hydraulic Leaks Detected (No Leaks Detected, Minor Seepage, Active Leak Detected)
[ ] Hydraulic Pressure Reading (PSI)
[ ] Pit Debris and Cleanliness Observations
[ ] Photo of Hydraulic Cylinder/Hoses
[ ] Inspector Signature

--- DOCK DOOR AND HARDWARE ASSESSMENT ---
[ ] Door Operation Status (Operational, Requires Repair, Non-Functional)
[ ] Hardware Components Inspected (Tracks and Rollers, Springs and Cables, Torsion Bar, Weather Stripping/Seals, Door Opener/Motor)
[ ] Deficiency Details
[ ] Photo Evidence of Hardware Condition
[ ] Inspector Authorization

--- SAFETY FEATURES AND COMMUNICATION ---
[ ] Dock Light Functionality (Green Light Operational, Red Light Operational, Faulty/Non-Operational)
[ ] Dock Lock/Vehicle Restraint Status (Fully Functional, Malfunctioning, Needs Maintenance)
[ ] Safety Equipment Present (Safety Chains, Safety Cones, Emergency Stop Buttons, Reflective Warning Signs)
[ ] Safety Deficiencies Identified
[ ] Photo Evidence of Safety Hazards
[ ] Inspector Verification

--- DOCK PLATE LIP AND DEPLOYMENT MECHANISM ---
[ ] Lip Deployment Status (Fully Functional, Partial Obstruction, Non-Functional/Malfunctioning)
[ ] Lip Extension Measurement (Inches)
[ ] Observed Mechanical Issues (Hinge Friction, Deformed Lip Edge, Mechanism Jamming, Structural Cracks)
[ ] Maintenance Notes/Observations
[ ] Photo of Deployment Mechanism
[ ] Last Inspection Date

--- ENVIRONMENTAL AND FLOOR CONDITIONS ---
[ ] Floor Surface Condition (Clean and Dry, , Debris Present, Cracked/Damaged)
[ ] Identified Hazards (Spill/Leak, Loose Debris, Obstruction in Dock Path, Inadequate Lighting)
[ ] Hazard Mitigation Actions Taken
[ ] Photos of Floor Condition
[ ] Inspector Verification
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