MASONRY JOINT INSPECTION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL INFORMATION ---
[ ] Project Name
[ ] Project Address
[ ] Inspection Date
[ ] Inspection Time
[ ] Inspector Name
[ ] Company Name (Inspector)
[ ] Temperature (Â°C/Â°F)
[ ] Weather Conditions (Clear, Cloudy, Rain, Snow, Fog)

--- VISUAL INSPECTION OF JOINTS ---
[ ] Joint Color Uniformity? (Uniform, Slight Variation, Significant Variation)
[ ] Joint Alignment? (Straight and Uniform, Minor Deviations, Significant Misalignment)
[ ] Presence of Cracking? (No Cracking, Hairline Cracks, Vertical Cracks, Horizontal Cracks, Map Cracking)
[ ] Description of Joint Condition (if not uniform or showing cracks)
[ ] Evidence of Efflorescence? (None, Slight, Moderate, Severe)
[ ] Joint Shape? (Concave, Flush, V-Joint, Other (Specify))
[ ] Describe any other unusual visual characteristics
[ ] Upload Visual Inspection Photos (if applicable)

--- JOINT TYPE AND MATERIAL VERIFICATION ---
[ ] Specified Joint Type (Raked, Flush, Weathered, Concave, Other (Specify))
[ ] If 'Other' Specified Above, Please Detail Joint Type
[ ] Specified Joint Mortar Type (Type N, Type S, Type M, Other (Specify))
[ ] If 'Other' Specified Above, Please Detail Mortar Type
[ ] Mortar Mix Ratio (Cement:Lime:Sand)
[ ] Mortar Specification Sheet (Optional)
[ ] Confirm joint type and material matches specifications? (Yes, No)
[ ] If 'No' Selected Above, Provide Details

--- EVIDENCE OF JOINT DETERIORATION ---
[ ] Type of Deterioration Observed (Check all that apply) (Cracking (Vertical), Cracking (Horizontal), Cracking (Diagonal), Pop-outs, Recessed Joints, Discoloration, Efflorescence, Scaling/Spalling, Honeycombing, Loss of Joint Material)
[ ] Maximum Crack Width (mm)
[ ] Description of Deterioration (Location, extent, pattern)
[ ] Number of Affected Joints (within inspected area)
[ ] Severity of Deterioration (Overall) (Minor, Moderate, Severe)
[ ] Photos of Deteriorated Joints
[ ] GPS Location of Deterioration (if applicable)

--- WATER PENETRATION ASSESSMENT ---
[ ] Was a water test (e.g., hose test, spray rack) performed? (Yes, No)
[ ] If yes to water test, what was the water pressure (PSI)?
[ ] Duration of water test (minutes)
[ ] Describe the method used for the water penetration assessment.
[ ] Evidence of active water penetration observed? (Yes, No, Uncertain)
[ ] If yes to water penetration, describe the location and nature of the penetration (e.g., staining, efflorescence, dripping).
[ ] Upload photos/videos documenting water penetration (if applicable).
[ ] Joint sealant condition related to water resistance? (Intact & Effective, Cracked/Damaged, Missing, Unknown)

--- STRUCTURAL INTEGRITY CONSIDERATIONS ---
[ ] Does joint deterioration appear to compromise structural stability? (Yes, No, Uncertain)
[ ] Describe any observations relating to masonry movement or displacement.
[ ] Estimated crack width (in mm) observed near joints (if any).
[ ] Is there evidence of bowing or leaning of masonry units? (Yes, No, Uncertain)
[ ] Describe any connection issues between masonry and supporting structure.
[ ] Is there evidence of differential settlement affecting joint performance? (Yes, No, Uncertain)
[ ] Upload supporting photos of structural concerns (if any).

--- DOCUMENTATION AND RECOMMENDATIONS ---
[ ] Summary of Findings
[ ] Detailed Recommendations for Repair/Maintenance
[ ] Estimated Cost of Recommended Repairs (USD)
[ ] Date of Next Recommended Inspection
[ ] Severity of Joint Condition (Overall) (Minor, Moderate, Significant, Critical)
[ ] Supporting Photographs (Joints, Damage, etc.)
[ ] Inspector Name
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/construction/masonry-joint-inspection-checklist
(Click "Install Template" to launch your digital inspection tool immediately)