NEW PRODUCT INTRODUCTION (NPI) MANUFACTURING WORKFLOW

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Initial Design Specifications: Fetch initial design specifications from the product design data model.
[ ] Assign Design Review Task: Create a task for the engineering team to review the design specifications.
[ ] Create Preliminary Bill of Materials (BOM): Create a preliminary BOM based on the design specifications.
[ ] Create Process Flow Diagram: Create a preliminary process flow diagram outlining the manufacturing steps.
[ ] Factory Feasibility Assessment Task: Assign a task to assess manufacturing feasibility at the factory.
[ ] Send Initial NPI Kickoff Email: Send an email to relevant stakeholders announcing the NPI process initiation.
[ ] Create Prototype Production Plan: Define the prototype production plan, including quantity and timeline.
[ ] Prototype Build Task Assignment: Assign the prototype build task to the manufacturing team.
[ ] Update BOM with Prototype Feedback: Update the BOM based on feedback from the prototype build.
[ ] Retrieve Prototype Test Results: Fetch the test results from the prototype testing phase.
[ ] Generate Prototype Test Report: Create a report summarizing the prototype test results.
[ ] Process Validation Task Assignment: Assign the task of validating the manufacturing process.
[ ] Update Manufacturing Instructions: Update manufacturing instructions with process validation findings.
[ ] Send NPI Launch Notification: Send an SMS notification to key personnel regarding the product launch.
[ ] Create Production Ramp-Up Plan: Define the plan for scaling up production volume.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/manufacturing/new-product-introduction-npi-manufacturing-workflow
(Click "Install Template" to launch your digital inspection tool immediately)