OIL AND GAS PIPELINE INSPECTION CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-INSPECTION PLANNING ---
[ ] Scheduled Inspection Date
[ ] Scheduled Inspection Start Time
[ ] Pipeline Segment Number/ID
[ ] Inspection Start Location (GPS Coordinates)
[ ] Ambient Temperature (°C)
[ ] Weather Conditions (Sunny, Cloudy, Rainy, Snowy, Foggy)
[ ] Review Relevant Maps/Diagrams (Upload)

--- RIGHT-OF-WAY & EXTERNAL CONDITIONS ---
[ ] Weather Conditions (Temperature °C)
[ ] Vegetation Condition (Excellent, Good, Fair, Poor)
[ ] Description of Vegetation Type
[ ] Potential Encroachments Observed? (Structures, Fences, Agriculture, None)
[ ] Location of Encroachment (if any)
[ ] Signage Condition
[ ] Date of last Right-of-Way clearing
[ ] Photos of Right-of-Way

--- PIPELINE PHYSICAL CONDITION ---
[ ] Pipeline Diameter (inches)
[ ] Pipeline Material (Carbon Steel, Stainless Steel, Composite, Other)
[ ] Corrosion Observed? (Yes, No, Unsure)
[ ] Description of any Corrosion (Location, Type, Severity)
[ ] Length of any cracks or seam failures (feet)
[ ] Photos of Physical Damage/Corrosion
[ ] Presence of Discoloration? (Yes, No, Unsure)
[ ] Description of Discoloration (Color, Location)

--- PIPELINE INTEGRITY COMPONENTS ---
[ ] Valve Operating Pressure (PSI)
[ ] Valve Condition (Excellent, Good, Fair, Poor)
[ ] Valve Comments/Observations
[ ] Pig Trap Depth (Feet)
[ ] Pig Trap Accessibility (Excellent, Good, Fair, Poor)
[ ] Pig Trap Photo (if applicable)
[ ] Last Pigging Date
[ ] Component Anomalies Observed (Check all that apply) (Corrosion, Damage, Erosion, Leaks, Other)

--- CATHODIC PROTECTION (CP) MONITORING ---
[ ] Near-Pipeline Potential (Volts)
[ ] Far-Pipeline Potential (Volts)
[ ] CP Current Output (Amps)
[ ] Rectifier Voltage (Volts)
[ ] Rectifier Status (Operating, Faulted, Standby)
[ ] Last Rectifier Maintenance Date
[ ] Notes on CP System Performance
[ ] Anode Condition (Good, Fair, Poor)

--- LEAK DETECTION SYSTEM (LDS) ASSESSMENT ---
[ ] Ambient Temperature (°C)
[ ] Pipeline Pressure (PSI)
[ ] LDS Sensitivity Setting
[ ] LDS Operational Status (Operational, Standby, Faulted)
[ ] Description of any alarms or events
[ ] Detector Calibration Status (Within Tolerance, Out of Tolerance, N/A)
[ ] Last Calibration Date

--- EROSION CONTROL MEASURES ---
[ ] GPS Coordinates of Erosion Area (if applicable)
[ ] Depth of Rill/Gully (inches)
[ ] Erosion Control Methods Present (Riprap, Vegetation (grass, trees), Silt Fences, Terracing, None)
[ ] Condition of Vegetation (Excellent, Good, Fair, Poor)
[ ] Detailed Observations of Erosion Control Measures
[ ] Width of Silt Fence (feet)
[ ] Effectiveness of Measures (Highly Effective, Effective, Partially Effective, Not Effective)

--- DOCUMENTATION AND REPORTING ---
[ ] Inspection Temperature (°C)
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Detailed Observations & Anomalies
[ ] Severity of Findings (Select all that apply) (Minor, Moderate, Major, Critical)
[ ] Overall Inspection Result (Satisfactory, Needs Repair, Unsafe - Immediate Action Required)
[ ] Supporting Photos/Videos
[ ] Inspector Name
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/inspection-management/oil-and-gas-pipeline-inspection-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)