OPEN-PIT MINING OPERATIONAL PLANNING

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Mine Plan Parameters: Fetch current production targets, pit boundaries, and geological constraints from the Mine Plan data model.
[ ] Get Equipment Availability: Retrieve real-time status and availability of shovels, trucks, and drills from the Fleet Management data model.
[ ] Calculate Required Fleet Capacity: Execute formula to determine the number of haul trucks needed based on total tonnage target and cycle time estimates.
[ ] Fetch Geotechnical Constraints: Retrieve slope stability limits and safety factor requirements from the Geotechnical data model.
[ ] Calculate Ore vs. Waste Ratio: Calculate the stripping ratio by dividing the volume of waste material by the volume of ore identified in the plan.
[ ] Draft Weekly Production Schedule: Assign task to Mine Planner to create the detailed daily/weekly extraction sequence.
[ ] Create Draft Mine Schedule: Generate a new entry in the 'Operational Schedules' data model containing the proposed plan.
[ ] Geotechnical Review: Assign task to Geotechnical Engineer to validate the proposed pit slope angles in the new schedule.
[ ] Update Pit Design Status: Update the status of the Pit Design entry to 'Review Complete' once safety checks are passed.
[ ] Fleet Dispatch Assignment: Assign task to Dispatcher to allocate specific machines to the newly defined loading zones.
[ ] Aggregate Weekly Tonnage Forecast: Sum the 'Estimated Tonnage' from all daily schedule entries to calculate total weekly production target.
[ ] Finalize Operational Plan: Assign task to Mine Manager for final approval and authorization of the weekly plan.
[ ] Notify Operations Team: Send an email to all Shift Supervisors containing the finalized production targets and pit maps.
[ ] Generate Weekly Plan Comparison: Create a report comparing the new Operational Plan against the Long-Term Mine Plan (LTMP) deviations.
[ ] Commit Plan to Master Schedule: Update the Master Mine Schedule entry with the approved weekly parameters.
[ ] Emergency Alert: Pit Boundary Change: Send SMS to all heavy equipment operators if the plan involves immediate changes to high-risk exclusion zones.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/mining-management/open-pit-mining-operational-planning
(Click "Install Template" to launch your digital inspection tool immediately)