PARKING LOT SAFETY & LIGHTING INSPECTION CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL AREA ASSESSMENT ---
[ ] Lot Size (Square Feet)
[ ] Lot Surface Type (Asphalt, Concrete, Gravel, Other)
[ ] Describe general condition of the lot (e.g., cracks, potholes, overall cleanliness)
[ ] Evidence of Standing Water? (Yes, No, N/A)
[ ] Landscaping Issues Observed? (Overgrown Vegetation, Dead/Diseased Plants, Poor Drainage, None)
[ ] Location of any noticeable concerns (e.g., overgrown vegetation)

--- LIGHTING ASSESSMENT ---
[ ] Lux Level at Entrance (Foot Candles)
[ ] Lux Level at Aisles (Foot Candles)
[ ] Lux Level at Parking Spaces (Foot Candles)
[ ] Lighting Uniformity (Excellent, Good, Fair, Poor)
[ ] Lights Not Functioning? (Yes - Broken Lens, Yes - Burned Out Bulb, Yes - Wiring Issue, No)
[ ] Notes on Lighting Issues/Observations
[ ] Last Maintenance Date

--- PAVEMENT & SURFACE CONDITION ---
[ ] Presence of Potholes (count)
[ ] Pavement Cracking Severity (None, Minor (hairline cracks), Moderate (larger cracks, some surface raveling), Severe (extensive cracking, significant surface loss))
[ ] Surface Condition - Overall (Good, Fair, Poor)
[ ] Number of Visible Oil/Fluid Stains
[ ] Describe any unusual pavement deterioration or damage
[ ] Presence of Trip Hazards (e.g., raised sections, uneven surfaces) (Yes, No)
[ ] Depth of Deepest Pothole (in inches)

--- SIGNAGE & MARKINGS ---
[ ] Are parking signs clearly visible and legible? (Yes, No, N/A)
[ ] Are directional arrows/markings clear and understandable? (Yes, No, N/A)
[ ] Number of faded/damaged parking stall lines (estimate)
[ ] Describe any issues with parking signage (e.g., missing signs, incorrect information)
[ ] Are speed limit signs present and visible? (Yes, No, N/A)
[ ] Detail any discrepancies found between signage and actual parking conditions.

--- OBSTACLES & HAZARDS ---
[ ] Identify any visible cracks or potholes exceeding 2 inches in width. (Yes, minor cracks (less than 2 inches), Yes, cracks/potholes exceeding 2 inches, No visible cracks/potholes)
[ ] Are there any visible debris (e.g., trash, branches, construction materials)? (Yes, small debris (easily removable), Yes, large debris or obstructions, No debris present)
[ ] Measure the depth of any identified potholes (in inches).
[ ] Describe the nature and location of any other obstacles or hazards not covered above.
[ ] Are any trees or shrubs obstructing visibility?  (Yes, No)
[ ] Mark the location of any significant hazards on the parking lot map.
[ ] Upload photos of any observed hazards.

--- SECURITY FEATURES ---
[ ] Number of Security Cameras Present
[ ] Camera Functionality - Are Cameras Operational? (Yes, No, Partial - Some Not Working)
[ ] Presence of Bollards/Barriers? (Yes, No, Partial - Some Areas Protected)
[ ] Notes on Security Patrol Presence (if applicable)
[ ] Lighting Adjacent to Entrances - Adequate? (Yes, No, Needs Improvement)
[ ] Upload Photo of Security System Controls (if accessible)

--- ADA COMPLIANCE ---
[ ] Number of Designated Accessible Parking Spaces
[ ] Accessible Space Width (feet)
[ ] Accessible Route to Entrance Clear? (Yes, No, N/A)
[ ] Curb Ramps Present and Functional? (Yes, No, N/A)
[ ] Accessible Signage Present & Visible? (Yes, No, N/A)
[ ] Notes on ADA compliance issues or observations

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/retail/parking-lot-safety-lighting-inspection-checklist
(Click "Install Template" to launch your digital inspection tool immediately)