PLANTER SEED METER ADJUSTMENT

Created by ChecklistGuro (https://checklistguro.com)

--- PREPARATION & SAFETY ---
[ ] Operator Name
[ ] Date of Adjustment
[ ] Planter Model
[ ] Seed Meter Serial Number
[ ] PPE (Personal Protective Equipment) Verified? (Yes, No)
[ ] Notes on Site Conditions (e.g., terrain, weather)
[ ] Area Cleared of Obstructions? (Yes, No)

--- EQUIPMENT & TOOLS ---
[ ] Seed Meter Model (Model A, Model B, Model C, Other)
[ ] Manufacturer's Calibration Gauge (if applicable)
[ ] Seed Size Gauge/Micrometer (if applicable)
[ ] Tools Available (Screwdrivers (various sizes), Wrenches (various sizes), Calibration Gauge (specific to meter), Seed Counting Tray, Ruler/Measuring Tape, Gloves)
[ ] Photo of Tool Setup (Optional)
[ ] Notes on available tools and condition

--- VISUAL INSPECTION ---
[ ] Describe any visible damage to the seed meter housing.
[ ] Check for worn or cracked seed plates. Select all that apply. (No cracks or wear, Minor cracks/wear, Significant cracks/wear, Seed plate missing)
[ ] Count the number of visible foreign objects (debris, dirt, plant material) in the seed meter.
[ ] Are the seed cells clear of obstructions? (Yes, No, Partially Obstructed)
[ ] Note any unusual noises or movement during manual rotation of the seed meter.
[ ] Check for wear on seed drive components (rollers, gears). Select the best description. (No visible wear, Slight wear, Moderate wear, Significant wear)

--- SEED METER CALIBRATION SETUP ---
[ ] Seed Meter Operating Speed (MPH)
[ ] Seed Meter Type (e.g., Vacuum, Mechanical) (Vacuum, Mechanical, Other (Specify))
[ ] Reference Manufacturer's Calibration Procedure
[ ] Desired Population (Seeds/Acre)
[ ] Calibration Method (e.g., Field Test, Lab Test) (Field Test, Lab Test, Manufacturer's Procedure)
[ ] Seed Spacing Adjustment Increment (Inches)
[ ] Date of Calibration Setup

--- SEED SIZE & VARIETY VERIFICATION ---
[ ] Seed Variety (Corn, Soybean, Wheat, Canola, Other)
[ ] Seed Size (mm)
[ ] Seed Supplier Specifications
[ ] Seed Quality Grade (A, B, C, Ungraded)
[ ] Seed Analysis Report (Optional)

--- SEED METER ADJUSTMENT PROCEDURE ---
[ ] Adjust Seed Plate Position (mm)
[ ] Adjust Spacing Gauge Setting (inches)
[ ] Seed Cup Type (Standard Cup, Short Cup, Extended Cup)
[ ] Adjust Drive Gear Ratio (if applicable)
[ ] Notes on Specific Adjustment Techniques
[ ] Adjustment Method Used (per manufacturer's instructions) (Visual Adjustment, Weight Calibration, Electronic Calibration)
[ ] Seed Cup RPM (if applicable, measured)

--- POPULATION VERIFICATION & FINE-TUNING ---
[ ] Test Row Length (feet)
[ ] Number of Plants Counted
[ ] Actual Planted Population (plants/acre)
[ ] Target Planted Population (plants/acre)
[ ] Population Accuracy (Within Tolerance, Slightly High, Slightly Low, Outside Tolerance)
[ ] Adjustment Increment (e.g., seed plate rotation degrees)
[ ] Notes on Population Verification and Adjustments
[ ] Seed Type Used for Verification (Same as Planting, Different - Specify in Notes)

--- DOCUMENTATION & RECORD KEEPING ---
[ ] Date of Adjustment
[ ] Seed Meter Serial Number
[ ] Planted Population (Plants/Acre)
[ ] Seed Variety Used (Corn - X Variety, Soybean - Y Variety, Wheat - Z Variety, Other - Specify in Long Text)
[ ] Notes/Comments (e.g., specific adjustment issues, environmental conditions)
[ ] Meter Setting (as per manual)
[ ] Adjustment Performed By (Mechanic 1, Mechanic 2, Technician 1, Technician 2)

--- POST-ADJUSTMENT CHECKS & CLEAN-UP ---
[ ] Verify Population with Drop Test (Plants/Foot)
[ ] Meter Operation Observed (Smooth, Erratic, etc.) (Smooth, Erratic, Choppy, Uneven)
[ ] Notes on observed meter behavior during the verification process
[ ] Date of Verification
[ ] Time of Verification
[ ] Clean any Seed Debris? (Yes, No)
[ ] Technician Name
[ ] Equipment ID (If Applicable)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/agriculture/planter-seed-meter-adjustment
(Click "Install Template" to launch your digital inspection tool immediately)