POST-HARVEST GRAIN MOISTURE CONTENT

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-HARVEST CONSIDERATIONS ---
[ ] Expected Harvest Date (Day of Year)
[ ] Crop Variety Used (Influences Moisture Content) (Variety A, Variety B, Variety C, Other (Specify in Long Text))
[ ] Notes on Recent Weather Patterns (Drought, Rain, etc.)
[ ] Current Soil Moisture Levels (Scale of 1-10)
[ ] Management Practices Implemented (Select all that apply) (Controlled Irrigation, Fertilizer Application, Pest & Disease Control, Weed Management)
[ ] Date of Last Irrigation

--- HARVESTING & INITIAL HANDLING ---
[ ] Harvested Grain Volume (tons/bushels)
[ ] Harvest Method Used (Combine, Manual, Other (Specify))
[ ] Describe any unusual conditions during harvest (e.g., uneven ripening, weather)
[ ] Estimated Grain Moisture Content at Harvest (%)
[ ] Cleanliness of Grain at Harvest (Excellent, Good, Fair, Poor)
[ ] Foreign Materials Present? (Weeds, Stones, Dirt/Clay, Insect Damage, None)
[ ] Describe any observed damage to grain during harvesting or initial handling (e.g., breakage, bruising)

--- MOISTURE MEASUREMENT - EQUIPMENT & CALIBRATION ---
[ ] Moisture Meter Type Used? (Handheld Electric, Grain Bin Monitor, Near-Infrared (NIR) Sensor, Drive-Over Scale with Moisture Sensor, Other - Specify)
[ ] Manufacturer of Moisture Meter?
[ ] Model Number of Moisture Meter?
[ ] Last Calibration Date (YYYY-MM-DD)
[ ] Next Calibration Date Due (YYYY-MM-DD)
[ ] Calibration Standard Used (Moisture %)
[ ] Record of Calibration Readings (Standard vs. Meter Reading)
[ ] Calibration Verification Passed? (Yes, No, N/A)
[ ] If Calibration Failed, Describe Problem and Action Taken

--- GRAIN MOISTURE CONTENT ASSESSMENT ---
[ ] Grain Lot ID
[ ] Grain Type (Wheat, Corn, Soybean, Barley, Rice, Oats, Other (Specify in LONG_TEXT))
[ ] If 'Other' grain type selected, specify:
[ ] Moisture Measurement Method (Moisture Meter (Electrical), Moisture Meter (Capacitance), Oven Drying Method, Other (Specify in LONG_TEXT))
[ ] If 'Other' measurement method selected, specify:
[ ] Moisture Content (%) - Reading 1
[ ] Moisture Content (%) - Reading 2
[ ] Average Moisture Content (%)
[ ] Acceptable Moisture Content Range (According to standards) (Check local/regional standards, Not Applicable)
[ ] Comments/Observations (e.g., grain condition, meter readings, any anomalies)

--- STORAGE PREPARATION & SEALING ---
[ ] Storage Type (Grain Bin, Silo, Flat Storage, Other)
[ ] Bin/Silo Cleanliness Rating (1-10)
[ ] Pre-Storage Cleaning Procedures Completed? (Sweeping, Scraping, Washing, Insecticide Application, None)
[ ] Sealing Material Type (Tarpaulin, Grain Bags, Caulking, None)
[ ] Number of Roof/Wall Seam Leaks Identified
[ ] Description of Any Structural Damage (roof, walls, floor)
[ ] Ventilation System Operational? (Yes, No, Not Applicable)
[ ] Comments regarding storage preparation

--- MONITORING DURING STORAGE ---
[ ] Date of Moisture Content Check
[ ] Time of Moisture Content Check
[ ] Moisture Content (%)
[ ] Temperature (Â°C/Â°F)
[ ] Grain Condition (Appearance) (Excellent, Good, Fair, Poor)
[ ] Odor Presence (None, Fungi, Musty, Other)
[ ] Notes/Observations
[ ] Action Taken (if applicable) (None, Aeration, Temperature Adjustment, Re-stacking, Other)
[ ] Details of Action Taken (if applicable)

--- CORRECTIVE ACTIONS ---
[ ] Moisture Content Exceeds Limit: Initial Action (Increase Ventilation, Reduce Grain Mass (Removal), Apply Drying Strategy, Monitor Closely (No Immediate Action))
[ ] Target Moisture Content (Percentage)
[ ] Description of Drying Strategy Implemented
[ ] Airflow Rate (CFM) if applicable
[ ] Date of Corrective Action Initiated
[ ] Time of Corrective Action Initiated
[ ] Amount of Grain Removed (Kilograms/Pounds)
[ ] Reason for Moisture Exceedance (Incomplete Drying, Poor Ventilation, Leakage/Moisture Ingress, Unforeseen Weather Event, Other)
[ ] Additional Notes & Observations

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/agriculture/post-harvest-grain-moisture-content
(Click "Install Template" to launch your digital inspection tool immediately)