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--- PRE-OPERATIONAL INSPECTION ---
[ ] Inspection Date
[ ] Press Unit ID/Location
[ ] Machine Power Status (Fully Operational, Requires Maintenance, Emergency Shutdown Active)
[ ] Pre-Start Safety Checks Completed (Emergency Stops Tested, Guard Rails & Shields Secured, Area Clear of Debris, Personal Protective Equipment (PPE) Verified)
[ ] Visual Anomalies Noted
[ ] Inspector Signature

--- MECHANICAL & DRIVE SYSTEM CHECK ---
[ ] Drive Belt Tension Status (Adequate, Loose, Over-tightened, Requires Replacement)
[ ] Motor Temperature (°C)
[ ] Detected Anomalies (Excessive Vibration, Unusual Noise/Grinding, Slippage, Heat Discoloration)
[ ] Gear and Bearing Observations
[ ] Drive System Inspection Photo
[ ] Technician Verification

--- INKING & DAMPENING SYSTEM MAINTENANCE ---
[ ] Inspection Date
[ ] Ink Fountain Level Status (Adequate, Low - Needs Refill, Critical - Immediate Action Required)
[ ] Dampening Solution pH Level
[ ] Roller Condition Check (Clean, No Wear Detected, Resurfacing Needed, Replace Roller)
[ ] Roller Pressure & Impression Notes
[ ] Technician Verification

--- PAPER FEED & DELIVERY UNIT INSPECTION ---
[ ] Feeder Suction Pad Condition (Excellent, Good - Requires Cleaning, Worn - Needs Replacement, Damaged)
[ ] Gripper Timing Adjustment (mm)
[ ] Identified Issues (Paper Slippage, Misalignment, Debris in Delivery Tray, Sensor Malfunction, None)
[ ] Detailed Observations
[ ] Photo of Feeder Setup
[ ] Technician Verification

--- LUBRICATION & FLUID MANAGEMENT ---
[ ] Last Lubrication Date
[ ] Oil Level (Liters/Units)
[ ] Hydraulic Fluid Condition (Optimal, Needs Replenishment, Contaminated/Dirty, Critical/Low)
[ ] Completed Lubrication Points (Main Drive Bearings, Gearbox, Pneumatic Cylinders, Roller Bearings, Chain Drives)
[ ] Leakage Observations
[ ] Technician Approval

--- CLEANING & WASTE REMOVAL ---
[ ] Areas Cleaned (Ink Rollers, Plate Cylinders, Feeder Mechanism, Delivery Pile, Chassis/Machine Frame)
[ ] Debris/Waste Type Identified
[ ] Cleaning Notes & Residue Observations
[ ] Post-Cleaning Photo Documentation
[ ] Technician Verification

--- ELECTRICAL & CONTROL SYSTEM AUDIT ---
[ ] Audit Date
[ ] Emergency Stop Button Functionality (Operational, Faulty, Requires Repair)
[ ] Control Panel Display/HMI Status (Clear and Readable, Flickering/Unreadable, Error Codes Present)
[ ] Voltage Reading (Main Input)
[ ] Components Inspected (Circuit Breakers, Sensors & Limit Switches, Wiring Harnesses, Relays & Contactors, Capacitors)
[ ] Electrical Fault Observations
[ ] Technician Verification

--- PLATE & CYLINDER ALIGNMENT ---
[ ] Plate Mounting Integrity (Secure and Properly Aligned, Loose or Misaligned, Damaged/Requires Replacement)
[ ] Impression Cylinder Pressure (PSI)
[ ] Registration Error Measurement
[ ] Cylinder Surface Condition Notes
[ ] Technician Verification

--- POST-OPERATIONAL SHUTDOWN & DOCUMENTATION ---
[ ] Maintenance Completion Date
[ ] Shutdown Completion Time
[ ] Operational Status After Shutdown (Fully Operational, Operational with Issues Noted, Requires Immediate Repair)
[ ] Maintenance Notes & Observations
[ ] Upload Maintenance Log/Report Photo
[ ] Technician Signature
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