PRODUCTION DATA ANALYSIS & REPORTING WORKFLOW

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Production Data: Fetch raw production data from the MES system for the reporting period.
[ ] Calculate Total Output: Aggregate production entries to determine total units produced.
[ ] Calculate Defect Rate: Aggregate data on defective units to calculate the overall defect rate.
[ ] Calculate OEE: Calculate Overall Equipment Effectiveness (OEE) based on availability, performance, and quality data.
[ ] Create Summary Report Entry: Create a new entry in the 'Production Summary Reports' data model.
[ ] Update Performance Metrics: Update existing KPIs in the 'Production Performance' data model with the calculated values.
[ ] Assign Review Task to Supervisor: Create a task for the production supervisor to review the generated report.
[ ] Send Report to Stakeholders: Automatically email the report to relevant stakeholders (e.g., plant manager, quality team).
[ ] Generate Visual Dashboard: Create a visual dashboard summarizing key production metrics.
[ ] Fetch Downtime Events: Retrieve information about downtime events from the maintenance system.
[ ] Calculate Downtime Duration: Aggregate downtime event data to determine total downtime duration.
[ ] Calculate Yield Rate: Calculate yield rate based on good output and total input.
[ ] Log Report Generation: Update a log entry to record the report generation and its status.
[ ] Escalate Issues to Engineering: Create a task for the engineering team if critical thresholds are breached.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/manufacturing/production-data-analysis-reporting-workflow
(Click "Install Template" to launch your digital inspection tool immediately)