PRODUCTION LINE DOWNTIME ANALYSIS WORKFLOW

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Downtime Event Records: Fetch all downtime event records from the past 24 hours, including timestamp, line ID, and reason code.
[ ] Calculate Total Downtime per Line: Aggregate downtime event records, calculating the total downtime (in minutes) for each production line.
[ ] Assign Initial Investigation Task: Create a task assigned to the maintenance technician to begin initial investigation of lines with > 15 minutes downtime.
[ ] Update Event Status to 'Under Investigation': Update the status of downtime events on lines flagged for investigation to 'Under Investigation'.
[ ] Retrieve Machine Performance Data: Get recent performance data (speed, temperature, error codes) for machines experiencing downtime.
[ ] Calculate MTBF (Mean Time Between Failures): Calculate MTBF for affected machines using historical downtime data.
[ ] Assign Root Cause Analysis Task: Create a task for an engineer to perform root cause analysis if downtime exceeds a threshold (e.g., 30 minutes).
[ ] Create Root Cause Entry: Create an entry in the Root Cause data model, capturing the engineer's findings.
[ ] Assign Corrective Action Task: Create a task for the responsible team to implement corrective actions based on the root cause analysis.
[ ] Update Downtime Event with Root Cause: Update the downtime event record with the identified root cause.
[ ] Create Corrective Action Plan Entry: Create an entry in the Corrective Action Plan data model outlining the steps to prevent recurrence.
[ ] Notify Supervisor of Critical Downtime: Send an email to the production supervisor for downtime events exceeding a critical threshold (e.g., 1 hour).
[ ] Generate Downtime Summary Report: Create a report summarizing downtime events for the past week, including lines affected, reasons, and corrective actions.
[ ] Update Event Status to 'Resolved': Update the status of downtime event to 'Resolved' after corrective actions are completed.
[ ] Retrieve similar downtime events: Get a list of similar downtime events in the past to compare the root cause and preventative action

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/manufacturing/production-line-downtime-analysis-workflow
(Click "Install Template" to launch your digital inspection tool immediately)